Macros
Mode
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants
Collaboration diagram for Mode:

## Macros
#define | LL_AON_GPIO_MODE_INPUT ((uint32_t)0x0U)
| Select input mode. More...
#define | LL_AON_GPIO_MODE_OUTPUT ((uint32_t)0x1U)
| Select output mode. More...
#define | LL_AON_GPIO_MODE_MUX ((uint32_t)0x2U)
| Select mux peripheral mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_MODE_INPUT

#define LL_AON_GPIO_MODE_INPUT ((uint32_t)0x0U)

Select input mode.

Definition at line 132 of file gr55xx_ll_aon_gpio.h.

## ◆ LL_AON_GPIO_MODE_MUX

#define LL_AON_GPIO_MODE_MUX ((uint32_t)0x2U)

Select mux peripheral mode.

Definition at line 134 of file gr55xx_ll_aon_gpio.h.

## ◆ LL_AON_GPIO_MODE_OUTPUT

#define LL_AON_GPIO_MODE_OUTPUT ((uint32_t)0x1U)

Select output mode.

Definition at line 133 of file gr55xx_ll_aon_gpio.h.