Macros
I2S FIFO Level Max
Peripheral Driver » HAL Driver » I2S » Defines » I2S Exported Constants
Collaboration diagram for I2S FIFO Level Max:

## Macros
#define | I2S_TX_FIFO_LEVEL_MAX 16
| I2S TX FIFO Level Max Value More...
#define | I2S_RX_FIFO_LEVEL_MAX 16
| I2S RX FIFO Level Max Value More...

## Detailed Description

## Macro Definition Documentation

## ◆ I2S_RX_FIFO_LEVEL_MAX

#define I2S_RX_FIFO_LEVEL_MAX 16

I2S RX FIFO Level Max Value

Definition at line 246 of file gr55xx_hal_i2s.h.

## ◆ I2S_TX_FIFO_LEVEL_MAX

#define I2S_TX_FIFO_LEVEL_MAX 16

I2S TX FIFO Level Max Value

Definition at line 245 of file gr55xx_hal_i2s.h.