Macros
Read data endian mode
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants
Collaboration diagram for Read data endian mode:

## Macros
#define | LL_XQSPI_XIP_ENDIAN_BIG 0x00000000UL
| Read data in big endian More...
#define | LL_XQSPI_XIP_ENDIAN_LITTLE XQSPI_XIP_CFG_LE32
| Read data in little endian. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_XIP_ENDIAN_BIG

#define LL_XQSPI_XIP_ENDIAN_BIG 0x00000000UL

Read data in big endian

Definition at line 169 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_XIP_ENDIAN_LITTLE

#define LL_XQSPI_XIP_ENDIAN_LITTLE XQSPI_XIP_CFG_LE32

Read data in little endian.

Definition at line 170 of file gr55xx_ll_xqspi.h.