Macros
Block2 Clock During WFI
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants
Collaboration diagram for Block2 Clock During WFI:

## Macros
#define | LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK
| Div4 clk for security blocks. More...
#define | LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK
| Div4 clk for xf qspi More...
#define | LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)
| All clock group 2 More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_WFI_ALL_HCLK2

#define LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)

All clock group 2

Definition at line 146 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_SECU_DIV4_PCLK

#define LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK

Div4 clk for security blocks.

Definition at line 143 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_XQSPI_DIV4_PCLK

#define LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK

Div4 clk for xf qspi

Definition at line 144 of file gr55xx_ll_cgc.h.