Enumerations
HAL HMAC state
Peripheral Driver » HAL Driver » HMAC » Enumerations

## Enumerations
enum | hal_hmac_state_t { HAL_HMAC_STATE_RESET = 0x00, HAL_HMAC_STATE_READY = 0x01, HAL_HMAC_STATE_BUSY = 0x02, HAL_HMAC_STATE_ERROR = 0x03, HAL_HMAC_STATE_TIMEOUT = 0x04, HAL_HMAC_STATE_SUSPENDED = 0x05 }
| HAL HMAC State enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_hmac_state_t

enum hal_hmac_state_t

HAL HMAC State enumerations definition.

Note
  HAL HMAC State value is a combination of 2 different substates: gState and RxState.

Enumerator
HAL_HMAC_STATE_RESET | Peripheral not initialized
HAL_HMAC_STATE_READY | Peripheral initialized and ready for use
HAL_HMAC_STATE_BUSY | Peripheral in indirect mode and busy
HAL_HMAC_STATE_ERROR | Peripheral in error
HAL_HMAC_STATE_TIMEOUT | Peripheral in timeout
HAL_HMAC_STATE_SUSPENDED | Peripheral in suspended

Definition at line 76 of file gr55xx_hal_hmac.h.