Public Attributes | List of all members
_wdt_init Struct Reference
Peripheral Driver » HAL Driver » WDT » Structures » WDT Configuration

WDT init structure definition. More...

`#include <gr55xx_hal_wdt.h>`

## Public Attributes
uint32_t | counter
uint32_t | reset_mode

## Detailed Description

WDT init structure definition.

Definition at line 75 of file gr55xx_hal_wdt.h.

## Member Data Documentation

## ◆ counter

uint32_t _wdt_init::counter

Specifies the WDT free-running downcounter value. This parameter can be a number ranging between 0x0U and 0xFFFFFFFFU.

Definition at line 77 of file gr55xx_hal_wdt.h.

## ◆ reset_mode

uint32_t _wdt_init::reset_mode

Specifies if WDT Reset output is enable or not. When RESET Mode is enabled, WDT will generate an interrupt on first timeout. If interrupt has not been cleared before the second timeout, WDT will then request a SoC Reset.

This parameter can be a value of WDT Reset Mode.

Definition at line 80 of file gr55xx_hal_wdt.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_wdt.h