Functions
IT_Management
Peripheral Driver » LL Driver » AES » Functions

## Functions
__STATIC_INLINE void | ll_aes_enable_it_done (aes_regs_t *AESx)
| Enable AES the done interrupt. More...
__STATIC_INLINE void | ll_aes_disable_it_done (aes_regs_t *AESx)
| Disable AES the done interrupt. More...
__STATIC_INLINE uint32_t | ll_aes_is_enabled_it_done (aes_regs_t *AESx)
| Indicate whether the done interrupt is enabled. More...

## Detailed Description

## Function Documentation

## ◆ ll_aes_disable_it_done()

__STATIC_INLINE void ll_aes_disable_it_done | ( | aes_regs_t * | AESx | ) |

Disable AES the done interrupt.

\rst +———————-+—————————–+ | Register | BitsName | +======================+=============================+ | INTERRUPT | ENABLE | +———————-+—————————–+ \endrst

Parameters

  AESx | AES instance

Return values

  None |

Definition at line 756 of file gr55xx_ll_aes.h.

## ◆ ll_aes_enable_it_done()

__STATIC_INLINE void ll_aes_enable_it_done | ( | aes_regs_t * | AESx | ) |

Enable AES the done interrupt.

\rst +———————-+—————————–+ | Register | BitsName | +======================+=============================+ | INTERRUPT | ENABLE | +———————-+—————————–+ \endrst

Parameters

  AESx | AES instance

Return values

  None |

Definition at line 737 of file gr55xx_ll_aes.h.

## ◆ ll_aes_is_enabled_it_done()

__STATIC_INLINE uint32_t ll_aes_is_enabled_it_done | ( | aes_regs_t * | AESx | ) |

Indicate whether the done interrupt is enabled.

\rst +———————-+—————————–+ | Register | BitsName | +======================+=============================+ | INTERRUPT | ENABLE | +———————-+—————————–+ \endrst

Parameters

  AESx | AES instance

Return values

  State | of bit (1 or 0).

Definition at line 775 of file gr55xx_ll_aes.h.