Macros
Characteristics Mask
BLE Services » Current Time Service (CTS) » Defines

Bit masks for the initialization of cts_init_t::char_mask. More...

## Macros
#define | CTS_CHAR_MANDATORY 0x0f
#define | CTS_CHAR_LOC_TIME_INFO_SUP 0x30
#define | CTS_CHAR_REF_TIME_INFO_SUP 0xc0
#define | CTS_CHAR_FULL 0xff

## Detailed Description

Bit masks for the initialization of cts_init_t::char_mask.

## Macro Definition Documentation

## ◆ CTS_CHAR_FULL

#define CTS_CHAR_FULL 0xff

Bit mask of the full characteristic.

Definition at line 92 of file cts.h.

## ◆ CTS_CHAR_LOC_TIME_INFO_SUP

#define CTS_CHAR_LOC_TIME_INFO_SUP 0x30

Bit mask for Local Time Information characteristic that is optional.

Definition at line 90 of file cts.h.

## ◆ CTS_CHAR_MANDATORY

#define CTS_CHAR_MANDATORY 0x0f

Bit mask for mandatory characteristic in CTS.

Definition at line 89 of file cts.h.

## ◆ CTS_CHAR_REF_TIME_INFO_SUP

#define CTS_CHAR_REF_TIME_INFO_SUP 0xc0

Bit mask for Reference Time Information characteristic that is optional.

Definition at line 91 of file cts.h.