Macros
TX FIFO Threshold
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_TX_FIFO_TH_EMPTY 0x00000000U
#define | LL_I2C_TX_FIFO_TH_CHAR_1 0x00000001U
#define | LL_I2C_TX_FIFO_TH_CHAR_2 0x00000002U
#define | LL_I2C_TX_FIFO_TH_CHAR_3 0x00000003U
#define | LL_I2C_TX_FIFO_TH_CHAR_4 0x00000004U
#define | LL_I2C_TX_FIFO_TH_CHAR_5 0x00000005U
#define | LL_I2C_TX_FIFO_TH_CHAR_6 0x00000006U
#define | LL_I2C_TX_FIFO_TH_CHAR_7 0x00000007U

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_TX_FIFO_TH_CHAR_1

#define LL_I2C_TX_FIFO_TH_CHAR_1 0x00000001U

1 character in TX FIFO

Definition at line 222 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_2

#define LL_I2C_TX_FIFO_TH_CHAR_2 0x00000002U

2 characters in TX FIFO

Definition at line 223 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_3

#define LL_I2C_TX_FIFO_TH_CHAR_3 0x00000003U

3 characters in TX FIFO

Definition at line 224 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_4

#define LL_I2C_TX_FIFO_TH_CHAR_4 0x00000004U

4 characters in TX FIFO

Definition at line 225 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_5

#define LL_I2C_TX_FIFO_TH_CHAR_5 0x00000005U

5 characters in TX FIFO

Definition at line 226 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_6

#define LL_I2C_TX_FIFO_TH_CHAR_6 0x00000006U

6 characters in TX FIFO

Definition at line 227 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_7

#define LL_I2C_TX_FIFO_TH_CHAR_7 0x00000007U

7 characters in TX FIFO

Definition at line 228 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_EMPTY

#define LL_I2C_TX_FIFO_TH_EMPTY 0x00000000U

TX FIFO empty

Definition at line 221 of file gr55xx_ll_i2c.h.