Public Attributes | List of all members
_aes_init Struct Reference
Peripheral Driver » HAL Driver » AES » Structures » AES Configuration

AES Init Structure definition. More...

`#include <gr55xx_hal_aes.h>`

## Public Attributes
uint32_t | key_size
uint32_t | operation_mode
uint32_t | chaining_mode
uint32_t * | p_key
uint32_t * | p_init_vector
uint32_t | dpa_mode
uint32_t * | p_seed

## Detailed Description

AES Init Structure definition.

Definition at line 100 of file gr55xx_hal_aes.h.

## Member Data Documentation

## ◆ chaining_mode

uint32_t _aes_init::chaining_mode

AES chaining mode. This parameter can be a value of AES Chaining Mode

Definition at line 108 of file gr55xx_hal_aes.h.

## ◆ dpa_mode

uint32_t _aes_init::dpa_mode

DPA Mode

Definition at line 116 of file gr55xx_hal_aes.h.

## ◆ key_size

uint32_t _aes_init::key_size

128, 192 or 256-bits key length. This parameter can be a value of AES Key Size

Definition at line 102 of file gr55xx_hal_aes.h.

## ◆ operation_mode

uint32_t _aes_init::operation_mode

AES operating mode. This parameter can be a value of AES Operation Mode

Definition at line 105 of file gr55xx_hal_aes.h.

## ◆ p_init_vector

uint32_t* _aes_init::p_init_vector

Initialization Vector used for CBC modes

Definition at line 114 of file gr55xx_hal_aes.h.

## ◆ p_key

uint32_t* _aes_init::p_key

Encryption/Decryption Key. Normally, it should be a global pointer.

Definition at line 111 of file gr55xx_hal_aes.h.

## ◆ p_seed

uint32_t* _aes_init::p_seed

Random seeds

Definition at line 118 of file gr55xx_hal_aes.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_aes.h