Macros
COMP INPUT SOURCE
Peripheral Driver » LL Driver » COMP » Defines » COMP Exported Constants

## Macros
#define | LL_COMP_INPUT_SRC_IO0 (0UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)
#define | LL_COMP_INPUT_SRC_IO1 (1UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)
#define | LL_COMP_INPUT_SRC_IO2 (2UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)
#define | LL_COMP_INPUT_SRC_IO3 (3UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)
#define | LL_COMP_INPUT_SRC_IO4 (4UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_COMP_INPUT_SRC_IO0

#define LL_COMP_INPUT_SRC_IO0 (0UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)

Set MSIO_0 as inputs for the comparator

Definition at line 112 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_INPUT_SRC_IO1

#define LL_COMP_INPUT_SRC_IO1 (1UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)

Set MSIO_1 as inputs for the comparator

Definition at line 113 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_INPUT_SRC_IO2

#define LL_COMP_INPUT_SRC_IO2 (2UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)

Set MSIO_2 as inputs for the comparator

Definition at line 114 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_INPUT_SRC_IO3

#define LL_COMP_INPUT_SRC_IO3 (3UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)

Set MSIO_3 as inputs for the comparator

Definition at line 115 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_INPUT_SRC_IO4

#define LL_COMP_INPUT_SRC_IO4 (4UL << AON_RF_REG_10_CHANNEL_SEL_P_Pos)

Set MSIO_4 as inputs for the comparator

Definition at line 116 of file gr55xx_ll_comp.h.