Functions
Initialization and de-initialization functions
Peripheral Driver » LL Driver » AES » Functions

## Functions
error_status_t | ll_aes_deinit (aes_regs_t *AESx)
| De-initialize AES registers (Registers restored to their default values). More...
error_status_t | ll_aes_init (aes_regs_t *AESx, ll_aes_init_t *p_aes_init)
| Initialize AES registers according to the specified parameters in p_aes_init. More...
void | ll_aes_struct_init (ll_aes_init_t *p_aes_init)
| Set each field of a ll_aes_init_t type structure to default value. More...

## Detailed Description

## Function Documentation

## ◆ ll_aes_deinit()

error_status_t ll_aes_deinit | ( | aes_regs_t * | AESx | ) |

De-initialize AES registers (Registers restored to their default values).

Parameters

  AESx | AES Instance

Return values

  An | error_status_t enumeration value: SUCCESS: AES registers are de-initialized ERROR: AES registers are not de-initialized

## ◆ ll_aes_init()

error_status_t ll_aes_init | ( | aes_regs_t * | AESx,
|  | ll_aes_init_t * | p_aes_init
| ) |  |

Initialize AES registers according to the specified parameters in p_aes_init.

Parameters

  AESx | AES Instance
  p_aes_init | Pointer to a ll_aes_init_t structure that contains the configuration information for the specified AES peripheral.

Return values

  An | error_status_t enumeration value: SUCCESS: AES registers are initialized according to p_aes_init content ERROR: Problem occurred during AES Registers initialization

## ◆ ll_aes_struct_init()

void ll_aes_struct_init | ( | ll_aes_init_t * | p_aes_init | ) |

Set each field of a ll_aes_init_t type structure to default value.

Parameters

  p_aes_init | Pointer to a ll_aes_init_t structure whose fields will be set to default values.

Return values

  None |