Macros
GPIO0_PIN10 MUX selection
Peripheral Driver » HAL Driver » GPIOEx » Defines » GPIOEx Exported Constants » GPIOEx Mux function selection

## Macros
#define | GPIO0_PIN10_MUX_I2SM_RX_SDI GPIO_MUX_0
#define | GPIO0_PIN10_MUX_I2SS_RX_SDI GPIO_MUX_1
#define | GPIO0_PIN10_MUX_UART0_TX GPIO_MUX_2
#define | GPIO0_PIN10_MUX_I2C0_SCL GPIO_MUX_4
#define | GPIO0_PIN10_MUX_PWM1_B GPIO_MUX_5
#define | GPIO0_PIN10_MUX_COEX_BLE_TX GPIO_MUX_6

## Detailed Description

## Macro Definition Documentation

## ◆ GPIO0_PIN10_MUX_COEX_BLE_TX

#define GPIO0_PIN10_MUX_COEX_BLE_TX GPIO_MUX_6

GPIO0_PIN10 Mux Select COEX_BLE_TX

Definition at line 229 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN10_MUX_I2C0_SCL

#define GPIO0_PIN10_MUX_I2C0_SCL GPIO_MUX_4

GPIO0_PIN10 Mux Select I2C0_SCL

Definition at line 227 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN10_MUX_I2SM_RX_SDI

#define GPIO0_PIN10_MUX_I2SM_RX_SDI GPIO_MUX_0

GPIO0_PIN10 Mux Select I2SM_RX_SDI

Definition at line 224 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN10_MUX_I2SS_RX_SDI

#define GPIO0_PIN10_MUX_I2SS_RX_SDI GPIO_MUX_1

GPIO0_PIN10 Mux Select I2SS_RX_SDI

Definition at line 225 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN10_MUX_PWM1_B

#define GPIO0_PIN10_MUX_PWM1_B GPIO_MUX_5

GPIO0_PIN10 Mux Select PWM1_B

Definition at line 228 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN10_MUX_UART0_TX

#define GPIO0_PIN10_MUX_UART0_TX GPIO_MUX_2

GPIO0_PIN10 Mux Select UART0_TX

Definition at line 226 of file gr55xx_hal_gpio_ex.h.