Macros
Defines
SYSTEM » System SDK

## Macros
#define | SYS_INVALID_TIMER_ID 0xFF
#define | SYS_BD_ADDR_LEN BLE_GAP_ADDR_LEN
#define | SYS_CHIP_UID_LEN 0x10
#define | SYS_SET_BD_ADDR(BD_ADDR_ARRAY) nvds_put(0xC001, SYS_BD_ADDR_LEN, BD_ADDR_ARRAY)
#define | SYS_ROM_VERSION_ADDR 0x45000

## Detailed Description

## Macro Definition Documentation

## ◆ SYS_BD_ADDR_LEN

#define SYS_BD_ADDR_LEN BLE_GAP_ADDR_LEN

Length of Bluetoth Device Address.

Definition at line 70 of file gr55xx_sys.h.

## ◆ SYS_CHIP_UID_LEN

#define SYS_CHIP_UID_LEN 0x10

Length of Bluetoth Chip UID.

Definition at line 71 of file gr55xx_sys.h.

## ◆ SYS_INVALID_TIMER_ID

#define SYS_INVALID_TIMER_ID 0xFF

Invalid system Timer ID.

Definition at line 69 of file gr55xx_sys.h.

## ◆ SYS_ROM_VERSION_ADDR

#define SYS_ROM_VERSION_ADDR 0x45000

The rom version address.

Definition at line 73 of file gr55xx_sys.h.

## ◆ SYS_SET_BD_ADDR

#define SYS_SET_BD_ADDR | ( |  | BD_ADDR_ARRAY | ) | nvds_put(0xC001, SYS_BD_ADDR_LEN, BD_ADDR_ARRAY)

NVDS put BD address.

Definition at line 72 of file gr55xx_sys.h.