Public Attributes | List of all members
ble_gap_per_sync_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Periodic advertising synchronization parameters. More...

`#include <ble_gapm.h>`

## Public Attributes
uint16_t | skip
uint16_t | sync_to
ble_gap_per_sync_type_t | type
uint8_t | rsvd
ble_gap_period_adv_addr_cfg_t | adv_addr

## Detailed Description

Periodic advertising synchronization parameters.

Definition at line 672 of file ble_gapm.h.

## Member Data Documentation

## ◆ adv_addr

ble_gap_period_adv_addr_cfg_t ble_gap_per_sync_param_t::adv_addr

Address of advertiser with which synchronization has to be established(used only if use_pal is false).

Definition at line 678 of file ble_gapm.h.

## ◆ rsvd

uint8_t ble_gap_per_sync_param_t::rsvd

Reserved for future use.

Definition at line 677 of file ble_gapm.h.

## ◆ skip

uint16_t ble_gap_per_sync_param_t::skip

Number of periodic advertising that can be skipped after a successful reception. Maximum authorized value is 499.

Definition at line 674 of file ble_gapm.h.

## ◆ sync_to

uint16_t ble_gap_per_sync_param_t::sync_to

Synchronization timeout for the periodic advertising (in unit of 10ms between 100ms and 163.84s).

Definition at line 675 of file ble_gapm.h.

## ◆ type

ble_gap_per_sync_type_t ble_gap_per_sync_param_t::type

Periodic synchronization type (see enum ble_gap_per_sync_type_t).

Definition at line 676 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h