Public Attributes | List of all members
_qspi_init_t Struct Reference
Peripheral Driver » HAL Driver » QSPI » Structures » QSPI Configuration

QSPI init Structure definition. More...

`#include <gr55xx_hal_qspi.h>`

## Public Attributes
uint32_t | clock_prescaler
uint32_t | clock_mode
uint32_t | rx_sample_delay

## Detailed Description

QSPI init Structure definition.

Definition at line 102 of file gr55xx_hal_qspi.h.

## Member Data Documentation

## ◆ clock_mode

uint32_t _qspi_init_t::clock_mode

Specifies the Clock Mode. It indicates the level that clock takes between commands. This parameter can be a value of QSPI Clock Mode

Definition at line 107 of file gr55xx_hal_qspi.h.

## ◆ clock_prescaler

uint32_t _qspi_init_t::clock_prescaler

Specifies the prescaler factor for generating clock based on the AHB clock. This parameter can be a number between 0 and 0xFFFF

Definition at line 104 of file gr55xx_hal_qspi.h.

## ◆ rx_sample_delay

uint32_t _qspi_init_t::rx_sample_delay

Specifies the RX sample delay. It is used to delay the sample of the RX input port. This parameter can be a number between 0 and 0x7

Definition at line 110 of file gr55xx_hal_qspi.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_qspi.h