Classes | Typedefs | Enumerations | Variables
Typedefs
SYSTEM » Power Manager

## Classes
struct | pwr_mgmt_var_box_t
| power manager setting parameter. Use pwr_mgmt_var_set to transfer the parameters in the structure to PMU, and then the pwr_mgmt_mode_set function will use the new parameters for power management. Note that this is an advanced API, the wrong setting of parameters may lead to abnormal power management, so please use it carefully. More...
struct | pwr_table_t
| parameter configuration table. More...

## Typedefs
typedef void(* | trace_func_t) (uint8_t)
| Trace function type. More...
typedef void(* | periph_func_t) (void)
| Peripheral function type. More...
typedef void(* | pwr_before_sleep_func_t) (void)
| Before sleep function type. More...
typedef pwr_mgmt_dev_state_t(* | pwr_dev_check_func_t) (void)
| Device check function type. More...
typedef void(* | io_dump_func_t) (void)
| function registered to dump io configuration. More...
typedef void(* | mem_check_proc_t) (void)
| mem check process type. More...

## Enumerations
enum | boot_mode_t { COLD_BOOT = 0, WARM_BOOT }
| power manager boot type. More...
enum | pwr_mgmt_mode_t { PMR_MGMT_ACTIVE_MODE = 0x0, PMR_MGMT_IDLE_MODE, PMR_MGMT_SLEEP_MODE }
| power manager model. More...
enum | pwr_mgmt_dev_state_t { DEVICE_BUSY = 0x0, DEVICE_IDLE }
| power manager device work state. More...
enum | notify_timer_event_t { EVENT_APP_TIMER_START = 0, EVENT_APP_TIMER_STOP }
| power manager app timer work state. More...
enum | { AMS_PLAYER_ATTR_ID_NAME, AMS_PLAYER_ATTR_ID_PLAYBACK_INFO, AMS_PLAYER_ATTR_ID_VOLUME, IAS_ALERT_NONE, IAS_ALERT_MILD, IAS_ALERT_HIGH, TRC_PWR_WFE_MODE = 0, TRC_PWR_DSLEEP_MODE, TRC_PWR_ACTIVE_MODE, TRC_PWR_BLE_RET_DSLEEP, TRC_PWR_APP_TIMER_REFUSE, TRC_PWR_APP_TIMER_PASS, TRC_PWR_BLE_TIMER_PASS, BIT_HCI_SEND_2_CONTROLLER, BIT_HAL_XQSPI_SET_XIP_PRESENT_STATUS, BIT_LL_XQSPI_INIT, BIT_HAL_EXFLASH_WRITE, BIT_HAL_EXFLASH_ERASE, BIT_HAL_EXFLASH_READ, BIT_BLE_BM_SET_SEC_INFO, BIT_KE_TASK_SCHEDULE }
| PMU Tracking. More...

## Variables
pwr_table_t | pwr_table []
| pwr table. More...

## Detailed Description

## Typedef Documentation

## ◆ io_dump_func_t

typedef void(* io_dump_func_t) (void)

function registered to dump io configuration.

Definition at line 145 of file gr55xx_pwr.h.

## ◆ mem_check_proc_t

typedef void(* mem_check_proc_t) (void)

mem check process type.

Definition at line 148 of file gr55xx_pwr.h.

## ◆ periph_func_t

typedef void(* periph_func_t) (void)

Peripheral function type.

Definition at line 136 of file gr55xx_pwr.h.

## ◆ pwr_before_sleep_func_t

typedef void(* pwr_before_sleep_func_t) (void)

Before sleep function type.

Definition at line 139 of file gr55xx_pwr.h.

## ◆ pwr_dev_check_func_t

typedef pwr_mgmt_dev_state_t(* pwr_dev_check_func_t) (void)

Device check function type.

Definition at line 142 of file gr55xx_pwr.h.

## ◆ trace_func_t

typedef void(* trace_func_t) (uint8_t)

Trace function type.

Definition at line 133 of file gr55xx_pwr.h.

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

PMU Tracking.

Enumerator
AMS_PLAYER_ATTR_ID_NAME | Player attribute index of name.
AMS_PLAYER_ATTR_ID_PLAYBACK_INFO | Player attribute index of playback information.
AMS_PLAYER_ATTR_ID_VOLUME | Player attribute index of volume.
IAS_ALERT_NONE | No alert.
IAS_ALERT_MILD | Mild alert.
IAS_ALERT_HIGH | High alert.
TRC_PWR_WFE_MODE | WFE mode.
TRC_PWR_DSLEEP_MODE | Deep sleep mode.
TRC_PWR_ACTIVE_MODE | Active mode.
TRC_PWR_BLE_RET_DSLEEP | BLE return deep sleep.
TRC_PWR_APP_TIMER_REFUSE | App timer refuse.
TRC_PWR_APP_TIMER_PASS | App timer pass.
TRC_PWR_BLE_TIMER_PASS | BLE timer pass.
BIT_HCI_SEND_2_CONTROLLER |
BIT_HAL_XQSPI_SET_XIP_PRESENT_STATUS |
BIT_LL_XQSPI_INIT |
BIT_HAL_EXFLASH_WRITE |
BIT_HAL_EXFLASH_ERASE |
BIT_HAL_EXFLASH_READ |
BIT_BLE_BM_SET_SEC_INFO |
BIT_KE_TASK_SCHEDULE |

Definition at line 108 of file gr55xx_pwr.h.

## ◆ boot_mode_t

enum boot_mode_t

power manager boot type.

Enumerator
COLD_BOOT | Cold boot state.
WARM_BOOT | Warm boot state.

Definition at line 79 of file gr55xx_pwr.h.

## ◆ notify_timer_event_t

enum notify_timer_event_t

power manager app timer work state.

Enumerator
EVENT_APP_TIMER_START | App-timer start state.
EVENT_APP_TIMER_STOP | App-timer stop state.

Definition at line 101 of file gr55xx_pwr.h.

## ◆ pwr_mgmt_dev_state_t

enum pwr_mgmt_dev_state_t

power manager device work state.

Enumerator
DEVICE_BUSY | Device busy state.
DEVICE_IDLE | Device idle state.

Definition at line 94 of file gr55xx_pwr.h.

## ◆ pwr_mgmt_mode_t

enum pwr_mgmt_mode_t

power manager model.

Enumerator
PMR_MGMT_ACTIVE_MODE | Full speed state.
PMR_MGMT_IDLE_MODE | Idle state.
PMR_MGMT_SLEEP_MODE | Deep sleep state.

Definition at line 86 of file gr55xx_pwr.h.

## Variable Documentation

## ◆ pwr_table

pwr_table_t pwr_table[]
| extern

pwr table.