Macros
RX FIFO Threshold
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_RX_FIFO_TH_CHAR_1 0x00000000U
#define | LL_I2C_RX_FIFO_TH_CHAR_2 0x00000001U
#define | LL_I2C_RX_FIFO_TH_CHAR_3 0x00000002U
#define | LL_I2C_RX_FIFO_TH_CHAR_4 0x00000003U
#define | LL_I2C_RX_FIFO_TH_CHAR_5 0x00000004U
#define | LL_I2C_RX_FIFO_TH_CHAR_6 0x00000005U
#define | LL_I2C_RX_FIFO_TH_CHAR_7 0x00000006U
#define | LL_I2C_RX_FIFO_TH_FULL 0x00000007U

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_RX_FIFO_TH_CHAR_1

#define LL_I2C_RX_FIFO_TH_CHAR_1 0x00000000U

1 character in RX FIFO

Definition at line 234 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_2

#define LL_I2C_RX_FIFO_TH_CHAR_2 0x00000001U

2 characters in RX FIFO

Definition at line 235 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_3

#define LL_I2C_RX_FIFO_TH_CHAR_3 0x00000002U

3 characters in RX FIFO

Definition at line 236 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_4

#define LL_I2C_RX_FIFO_TH_CHAR_4 0x00000003U

4 characters in RX FIFO

Definition at line 237 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_5

#define LL_I2C_RX_FIFO_TH_CHAR_5 0x00000004U

5 characters in RX FIFO

Definition at line 238 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_6

#define LL_I2C_RX_FIFO_TH_CHAR_6 0x00000005U

6 characters in RX FIFO

Definition at line 239 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_CHAR_7

#define LL_I2C_RX_FIFO_TH_CHAR_7 0x00000006U

7 characters in RX FIFO

Definition at line 240 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_RX_FIFO_TH_FULL

#define LL_I2C_RX_FIFO_TH_FULL 0x00000007U

RX FIFO full

Definition at line 241 of file gr55xx_ll_i2c.h.