Macros
Transfer Data width
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_DATASIZE_IGNORE (0x00000000UL)
#define | LL_I2S_DATASIZE_12BIT (1UL << I2S_RXSIZE_WLEN_Pos)
#define | LL_I2S_DATASIZE_16BIT (2UL << I2S_RXSIZE_WLEN_Pos)
#define | LL_I2S_DATASIZE_20BIT (3UL << I2S_RXSIZE_WLEN_Pos)
#define | LL_I2S_DATASIZE_24BIT (4UL << I2S_RXSIZE_WLEN_Pos)
#define | LL_I2S_DATASIZE_32BIT (5UL << I2S_RXSIZE_WLEN_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_DATASIZE_12BIT

#define LL_I2S_DATASIZE_12BIT (1UL << I2S_RXSIZE_WLEN_Pos)

Data size for I2S transfer: 12 bits

Definition at line 154 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_DATASIZE_16BIT

#define LL_I2S_DATASIZE_16BIT (2UL << I2S_RXSIZE_WLEN_Pos)

Data size for I2S transfer: 16 bits

Definition at line 155 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_DATASIZE_20BIT

#define LL_I2S_DATASIZE_20BIT (3UL << I2S_RXSIZE_WLEN_Pos)

Data size for I2S transfer: 20 bits

Definition at line 156 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_DATASIZE_24BIT

#define LL_I2S_DATASIZE_24BIT (4UL << I2S_RXSIZE_WLEN_Pos)

Data size for I2S transfer: 24 bits

Definition at line 157 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_DATASIZE_32BIT

#define LL_I2S_DATASIZE_32BIT (5UL << I2S_RXSIZE_WLEN_Pos)

Data size for I2S transfer: 32 bits

Definition at line 158 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_DATASIZE_IGNORE

#define LL_I2S_DATASIZE_IGNORE (0x00000000UL)

Data size for I2S transfer: 32 bits

Definition at line 153 of file gr55xx_ll_i2s.h.