Macros
GPIO0_PIN0 MUX selection
Peripheral Driver » HAL Driver » GPIOEx » Defines » GPIOEx Exported Constants » GPIOEx Mux function selection

## Macros
#define | GPIO0_PIN0_MUX_SWD_CLK GPIO_MUX_0
#define | GPIO0_PIN0_MUX_I2C0_SCL GPIO_MUX_1
#define | GPIO0_PIN0_MUX_I2C1_SCL GPIO_MUX_2
#define | GPIO0_PIN0_MUX_UART1_RTS GPIO_MUX_3
#define | GPIO0_PIN0_MUX_UART0_TX GPIO_MUX_4
#define | GPIO0_PIN0_MUX_UART1_TX GPIO_MUX_5
#define | GPIO0_PIN0_MUX_UART0_RTS GPIO_MUX_6

## Detailed Description

## Macro Definition Documentation

## ◆ GPIO0_PIN0_MUX_I2C0_SCL

#define GPIO0_PIN0_MUX_I2C0_SCL GPIO_MUX_1

GPIO0_PIN0 Mux Select I2C0_SCL

Definition at line 109 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN0_MUX_I2C1_SCL

#define GPIO0_PIN0_MUX_I2C1_SCL GPIO_MUX_2

GPIO0_PIN0 Mux Select I2C1_SCL

Definition at line 110 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN0_MUX_SWD_CLK

#define GPIO0_PIN0_MUX_SWD_CLK GPIO_MUX_0

GPIO0_PIN0 Mux Select SWD_CLK

Definition at line 108 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN0_MUX_UART0_RTS

#define GPIO0_PIN0_MUX_UART0_RTS GPIO_MUX_6

GPIO0_PIN0 Mux Select UART0_RTS

Definition at line 114 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN0_MUX_UART0_TX

#define GPIO0_PIN0_MUX_UART0_TX GPIO_MUX_4

GPIO0_PIN0 Mux Select UART0_TX

Definition at line 112 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN0_MUX_UART1_RTS

#define GPIO0_PIN0_MUX_UART1_RTS GPIO_MUX_3

GPIO0_PIN0 Mux Select UART1_RTS

Definition at line 111 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN0_MUX_UART1_TX

#define GPIO0_PIN0_MUX_UART1_TX GPIO_MUX_5

GPIO0_PIN0 Mux Select UART1_TX

Definition at line 113 of file gr55xx_hal_gpio_ex.h.