### - s -

- sample_location : gls_meas_val_t
- scan_dup_filt : ble_gap_scan_param_t
- scan_dup_filt_list_buf : stack_heaps_table_t
- scan_dup_filt_list_size : stack_heaps_table_t
- scan_intv : ble_gap_scan_wd_op_param_t
- scan_mode : ble_gap_scan_param_t
- scan_param_1m : ble_gap_ext_init_param_t , ble_gap_ext_scan_param_t
- scan_param_coded : ble_gap_ext_init_param_t , ble_gap_ext_scan_param_t
- scan_req : ble_gapm_evt_t
- scan_req_ind_en : ble_gap_adv_param_t
- scan_stop : ble_gapm_evt_t
- scan_type : ble_gap_scan_param_t
- scan_wd : ble_gap_scan_wd_op_param_t
- scl : app_i2c_pin_cfg_t
- sclk : app_i2s_pin_cfg_t
- sda : app_i2c_pin_cfg_t
- sdi : app_i2s_pin_cfg_t
- sdo : app_i2s_pin_cfg_t
- sdu_recv : ble_l2cap_evt_t
- sdu_send : ble_l2cap_evt_t
- sec : _calendar_handle , _calendar_time , prf_date_time_t
- sec_evt : ble_evt_t
- sec_lvl : ble_gap_lepsm_register_t
- second_cfg : ble_gap_ext_adv_param_t
- secure_mode : pkc_init_t
- security : _exflash_handle
- seed : _ll_rng_init
- seed_mode : _rng_init
- segm_num : uds_regi_user_data_stream_t
- segm_offset : uds_regi_user_data_stream_t
- sensor_loc : hrs_c_evt_t , hrs_init_t
- sensor_location : cscs_init_t , rscs_init_t
- sensor_status_annunciation : gls_meas_val_t
- seq_num : gls_racp_filter_t
- sequ_num : ags_header_base_t
- sequence_number : gls_meas_val_t
- serial_num_str : dis_init_t
- services : ble_gattc_evt_srvc_disc_t
- setting_info : thscps_evt_t
- setting_type : ths_evt_t
- shdl : ble_gatts_create_db_t
- shift_bits : _pkc_modular_shift
- shift_count : _pkc_handle
- signed_write : ble_gattc_write_no_resp_t
- silent : ancs_ntf_flags_t
- single_tx : ble_gap_set_pref_slave_evt_dur_param_t
- size : _mpu_region_init_t , app_i2c_evt_t , app_i2s_evt_t , app_iso7816_evt_t , app_qspi_evt_t , app_spi_evt_t , app_uart_evt_t
- skip : ble_gap_per_sync_param_t
- slave_addr : app_i2c_evt_t
- slave_latency : ble_gap_conn_param_t , ble_gap_conn_update_param_t , ble_gap_evt_conn_param_update_req_t , ble_gap_evt_conn_param_updated_t , ble_gap_evt_connected_t , ble_gap_init_param_t , gap_slv_pref_t
- slave_select : _ll_spim_init_t , _spi_init
- sleep_algo_dur : ble_slp_config_t
- sleep_enable : ble_slp_config_t
- slope_ext_1p0 : adc_trim_info_t
- slope_int_0p8 : adc_trim_info_t
- slope_int_1p2 : adc_trim_info_t
- slope_int_1p6 : adc_trim_info_t
- slope_int_2p0 : adc_trim_info_t
- slv_dev_addr : i2c_env_t
- soft_lean_mass : bcs_meas_val_t
- soft_lean_mass_present : bcs_meas_flag_t
- source : cts_c_ref_time_info_t , cts_ref_time_info_t
- speed : _i2c_init , _ll_i2c_init
- spi_abort_cplt_callback : _hal_spi_callback
- spi_dma_state : spi_env_t
- spi_env : app_spi_params_t
- spi_error_callback : _hal_spi_callback
- spi_msp_deinit : _hal_spi_callback
- spi_msp_init : _hal_spi_callback
- spi_rx_cplt_callback : _hal_spi_callback
- spi_state : spi_env_t
- spi_tx_cplt_callback : _hal_spi_callback
- spi_tx_rx_cplt_callback : _hal_spi_callback
- src_address : _ll_dma_init
- src_data_alignment : _dma_init
- src_data_width : _ll_dma_init
- src_increment : _dma_init
- src_increment_mode : _ll_dma_init
- src_peripheral : _ll_dma_init
- src_request : _dma_init
- srvc_browse : ble_gattc_evt_t
- srvc_perm : ble_gatts_create_db_t
- stage_update_source : cts_updata_ref_time_info_t
- start_flag : aes_env_t , hmac_env_t , i2c_env_t , i2s_env_t , iso7816_env_t , qspi_env_t , spi_env_t
- start_flush_flag : uart_env_t
- start_hdl : ble_gattc_browse_inc_srvc_t , ble_gattc_disc_char_t , ble_gattc_evt_browse_srvc_t , ble_gattc_include_t , ble_gattc_read_by_uuid_t , ble_gattc_service_t
- start_tx_flag : uart_env_t
- state : _adc_handle , _aes_handle , _calendar_handle , _comp_handle , _dma_handle , _dual_timer_handle , _efuse_handle , _exflash_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pkc_handle , _qspi_handle , _rng_handle , _spi_handle , _timer_handle , _xqspi_handle_t , pwm_handle_t
- status : ble_gatts_prep_write_cfm_t , ble_gatts_read_cfm_t , ble_gatts_write_cfm_t , gls_racp_rsp_t , prf_att_info_t , thscps_rsp_val_t
- step_calorie : wechat_pedo_meas_t
- step_count : wechat_pedo_meas_t , wechat_pedo_target_t
- step_count_target : wechat_init_t
- step_dist : wechat_pedo_meas_t
- stop_bits : _ll_uart_init_t , _uart_init
- str_info : ans_c_new_alert_t , ans_new_alert_t
- stream_id : ags_header_base_t , ags_stream_env_t
- string_data : ble_dis_c_read_rsp_t
- subregion_disable : _mpu_region_init_t
- sugg_dflt_data_len : ble_gap_dev_info_t
- suggted_max_tx_octets : ble_gap_sugg_dflt_data_len_t
- suggted_max_tx_time : ble_gap_sugg_dflt_data_len_t
- sup_new_alert_cat : ans_init_t
- sup_new_alert_cat_ids : ans_c_evt_t
- sup_timeout : ble_gap_conn_param_t , ble_gap_conn_update_param_t , ble_gap_evt_conn_param_update_req_t , ble_gap_evt_conn_param_updated_t , ble_gap_evt_connected_t , ble_gap_init_param_t
- sup_unread_alert_cat_ids : ans_c_evt_t
- sup_unread_alert_sta : ans_init_t
- supervision_to : ble_gap_ext_conn_param_t
- suppted_max_rx_octets : ble_gap_max_data_len_t
- suppted_max_rx_time : ble_gap_max_data_len_t
- suppted_max_tx_octets : ble_gap_max_data_len_t
- suppted_max_tx_time : ble_gap_max_data_len_t
- sw_rev_str : dis_init_t
- sync_cnt : dss_evt_t
- sync_dev_num : dss_evt_t
- sync_established : ble_gapm_evt_t
- sync_hdl : ble_gap_evt_sync_established_t
- sync_to : ble_gap_per_sync_param_t
- sys_id : ble_dis_c_read_rsp_t
- system_clk : dfu_boot_info_t
- systolic : bps_meas_t