Macros
Mode
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Exported Constants

## Macros
#define | LL_GPIO_MODE_INPUT ((uint32_t)0x0U)
#define | LL_GPIO_MODE_OUTPUT ((uint32_t)0x1U)
#define | LL_GPIO_MODE_MUX ((uint32_t)0x2U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_MODE_INPUT

#define LL_GPIO_MODE_INPUT ((uint32_t)0x0U)

Select input mode

Definition at line 141 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_MODE_MUX

#define LL_GPIO_MODE_MUX ((uint32_t)0x2U)

Select mux peripheral mode

Definition at line 143 of file gr55xx_ll_gpio.h.

## ◆ LL_GPIO_MODE_OUTPUT

#define LL_GPIO_MODE_OUTPUT ((uint32_t)0x1U)

Select output mode

Definition at line 142 of file gr55xx_ll_gpio.h.