Public Attributes | List of all members
cts_init_t Struct Reference
BLE Services » Current Time Service (CTS) » Structures

Current Time Service init structure. This contains all option and data needed for initialization of the service. More...

`#include <cts.h>`

## Public Attributes
cts_evt_handler_t | evt_handler
uint16_t | char_mask
cts_cur_time_t | cur_time
cts_loc_time_info_t | loc_time_info
cts_ref_time_info_t | ref_time_info

## Detailed Description

Current Time Service init structure. This contains all option and data needed for initialization of the service.

Definition at line 239 of file cts.h.

## Member Data Documentation

## ◆ char_mask

uint16_t cts_init_t::char_mask

Initial mask of supported characteristics, and configured with Characteristics Mask.

Definition at line 242 of file cts.h.

## ◆ cur_time

cts_cur_time_t cts_init_t::cur_time

Current Time.

Definition at line 243 of file cts.h.

## ◆ evt_handler

cts_evt_handler_t cts_init_t::evt_handler

Current Time Service event handler.

Definition at line 241 of file cts.h.

## ◆ loc_time_info

cts_loc_time_info_t cts_init_t::loc_time_info

Local Time information.

Definition at line 244 of file cts.h.

## ◆ ref_time_info

cts_ref_time_info_t cts_init_t::ref_time_info

Reference Time information.

Definition at line 245 of file cts.h.

The documentation for this struct was generated from the following file:

- cts.h