Functions
Initialization and de-initialization functions
Peripheral Driver » LL Driver » PKC » Functions

## Functions
error_status_t | ll_pkc_deinit (pkc_regs_t *PKCx)
| De-initialize PKC registers (Registers restored to their default values). More...
error_status_t | ll_pkc_init (pkc_regs_t *PKCx, ll_pkc_init_t *p_pkc_init)
| Initialize PKC registers according to the specified parameters in p_pkc_init. More...
void | ll_pkc_struct_init (ll_pkc_init_t *p_pkc_init)
| Set each field of a ll_pkc_init_t type structure to default value. More...

## Detailed Description

## Function Documentation

## ◆ ll_pkc_deinit()

error_status_t ll_pkc_deinit | ( | pkc_regs_t * | PKCx | ) |

De-initialize PKC registers (Registers restored to their default values).

Parameters

  PKCx | PKC Instance

Return values

  An | error_status_t enumeration value: SUCCESS: PKC registers are de-initialized ERROR: PKC registers are not de-initialized

## ◆ ll_pkc_init()

error_status_t ll_pkc_init | ( | pkc_regs_t * | PKCx,
|  | ll_pkc_init_t * | p_pkc_init
| ) |  |

Initialize PKC registers according to the specified parameters in p_pkc_init.

Parameters

  PKCx | PKC Instance
  p_pkc_init | pointer to a ll_pkc_init_t structure that contains the configuration information for the specified PKC peripheral.

Return values

  An | error_status_t enumeration value: SUCCESS: PKC registers are initialized according to p_pkc_init content ERROR: Problem occurred during PKC Registers initialization

## ◆ ll_pkc_struct_init()

void ll_pkc_struct_init | ( | ll_pkc_init_t * | p_pkc_init | ) |

Set each field of a ll_pkc_init_t type structure to default value.

Parameters

  p_pkc_init | pointer to a ll_pkc_init_t structure whose fields will be set to default values.

Return values

  None |