Macros
Category ID Bit Masks
BLE Services » Alert Notification Service Client (ANS_C) » Defines

Category ID Bit Masks. More...

## Macros
#define | ANS_C_SMPL_ALERT_SUP (0x01 << 0)
#define | ANS_C_EMAIL_SUP (0x01 << 1)
#define | ANS_C_NEWS_SUP (0x01 << 2)
#define | ANS_C_CALL_SUP (0x01 << 3)
#define | ANS_C_MISSED_CALL_SUP (0x01 << 4)
#define | ANS_C_SMS_MMS_SUP (0x01 << 5)
#define | ANS_C_VOICE_MAIL_SUP (0x01 << 6)
#define | ANS_C_SCHEDULE_SUP (0x01 << 7)
#define | ANS_C_HG_PRIO_ALERT_SUP (0x01 << 8)
#define | ANS_C_INSTANT_MES (0x01 << 9)
#define | ANS_C_ALL_CAT_SUP (0x03ff)

## Detailed Description

Category ID Bit Masks.

## Macro Definition Documentation

## ◆ ANS_C_ALL_CAT_SUP

#define ANS_C_ALL_CAT_SUP (0x03ff)

Bit for All Category Supported.

Definition at line 90 of file ans_c.h.

## ◆ ANS_C_CALL_SUP

#define ANS_C_CALL_SUP (0x01 << 3)

Bit for Call Supported.

Definition at line 83 of file ans_c.h.

## ◆ ANS_C_EMAIL_SUP

#define ANS_C_EMAIL_SUP (0x01 << 1)

Bit for Email Supported.

Definition at line 81 of file ans_c.h.

## ◆ ANS_C_HG_PRIO_ALERT_SUP

#define ANS_C_HG_PRIO_ALERT_SUP (0x01 << 8)

Bit for High Prioritized Alert Supported.

Definition at line 88 of file ans_c.h.

## ◆ ANS_C_INSTANT_MES

#define ANS_C_INSTANT_MES (0x01 << 9)

Bit for Instant Message Supported.

Definition at line 89 of file ans_c.h.

## ◆ ANS_C_MISSED_CALL_SUP

#define ANS_C_MISSED_CALL_SUP (0x01 << 4)

Bit for Missed Call Supported.

Definition at line 84 of file ans_c.h.

## ◆ ANS_C_NEWS_SUP

#define ANS_C_NEWS_SUP (0x01 << 2)

Bit for News Supported.

Definition at line 82 of file ans_c.h.

## ◆ ANS_C_SCHEDULE_SUP

#define ANS_C_SCHEDULE_SUP (0x01 << 7)

Bit for Schedule Supported.

Definition at line 87 of file ans_c.h.

## ◆ ANS_C_SMPL_ALERT_SUP

#define ANS_C_SMPL_ALERT_SUP (0x01 << 0)

Bit for Simple Alert Supported.

Definition at line 80 of file ans_c.h.

## ◆ ANS_C_SMS_MMS_SUP

#define ANS_C_SMS_MMS_SUP (0x01 << 5)

Bit for SMS/MMS Supported.

Definition at line 85 of file ans_c.h.

## ◆ ANS_C_VOICE_MAIL_SUP

#define ANS_C_VOICE_MAIL_SUP (0x01 << 6)

Bit for Voice Mail Supported.

Definition at line 86 of file ans_c.h.