Modules | Macros
Defines
BLE Services » Alert Notification Service Client (ANS_C)

## Modules
| Category ID Bit Masks
| Category ID Bit Masks.

## Macros
#define | ANS_C_CONNECTION_MAX 10
#define | ANS_C_ERROR_CMD_NOT_SUP 0xa0
#define | ANS_C_UTF_8_STR_LEN_MAX 18
#define | ANS_C_ALERT_NTF_CTRL_PT_VAL_LEN 2

## Detailed Description

## Macro Definition Documentation

## ◆ ANS_C_ALERT_NTF_CTRL_PT_VAL_LEN

#define ANS_C_ALERT_NTF_CTRL_PT_VAL_LEN 2

Length of Alert Notification Control Point value.

Definition at line 73 of file ans_c.h.

## ◆ ANS_C_CONNECTION_MAX

#define ANS_C_CONNECTION_MAX 10

Maximum number of HRS Client connections.

Definition at line 70 of file ans_c.h.

## ◆ ANS_C_ERROR_CMD_NOT_SUP

#define ANS_C_ERROR_CMD_NOT_SUP 0xa0

Command not supported.

Definition at line 71 of file ans_c.h.

## ◆ ANS_C_UTF_8_STR_LEN_MAX

#define ANS_C_UTF_8_STR_LEN_MAX 18

Maximum length of “UTF-8 string”.

Definition at line 72 of file ans_c.h.