Macros
Action state
Peripheral Driver » APP DRIVER » ISO7816 » Defines

## Macros
#define | APP_ISO7816_ACTION_NONE HAL_ISO7816_ACTION_NONE
#define | APP_ISO7816_ACTION_OFF HAL_ISO7816_ACTION_OFF
#define | APP_ISO7816_ACTION_STOPCLK HAL_ISO7816_ACTION_STOPCLK
#define | APP_ISO7816_ACTION_ON HAL_ISO7816_ACTION_ON
#define | APP_ISO7816_ACTION_WARMRST HAL_ISO7816_ACTION_WARMRST
#define | APP_ISO7816_ACTION_RX HAL_ISO7816_ACTION_RX
#define | APP_ISO7816_ACTION_TX HAL_ISO7816_ACTION_TX
#define | APP_ISO7816_ACTION_TXRX HAL_ISO7816_ACTION_TXRX

## Detailed Description

## Macro Definition Documentation

## ◆ APP_ISO7816_ACTION_NONE

#define APP_ISO7816_ACTION_NONE HAL_ISO7816_ACTION_NONE

Do Nothing.

Definition at line 73 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_OFF

#define APP_ISO7816_ACTION_OFF HAL_ISO7816_ACTION_OFF

Switch Off.

Definition at line 74 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_ON

#define APP_ISO7816_ACTION_ON HAL_ISO7816_ACTION_ON

Switch on and receive ATR.

Definition at line 76 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_RX

#define APP_ISO7816_ACTION_RX HAL_ISO7816_ACTION_RX

Receive.

Definition at line 78 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_STOPCLK

#define APP_ISO7816_ACTION_STOPCLK HAL_ISO7816_ACTION_STOPCLK

Stop the clock.

Definition at line 75 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_TX

#define APP_ISO7816_ACTION_TX HAL_ISO7816_ACTION_TX

Transmit.

Definition at line 79 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_TXRX

#define APP_ISO7816_ACTION_TXRX HAL_ISO7816_ACTION_TXRX

Transmit, followed by RX.

Definition at line 80 of file app_iso7816.h.

## ◆ APP_ISO7816_ACTION_WARMRST

#define APP_ISO7816_ACTION_WARMRST HAL_ISO7816_ACTION_WARMRST

Trigger warm reset and receive ATR.

Definition at line 77 of file app_iso7816.h.