Public Attributes | List of all members
pass_init_t Struct Reference
BLE Services » Phone Alert Status Service (PASS) » Structures

Phone Alert Status Service init stucture. This contains all option and data needed for initialization of the service. More...

`#include <pass.h>`

## Public Attributes
pass_evt_handler_t | evt_handler
uint16_t | char_mask
uint8_t | alert_status
uint8_t | ringer_setting

## Detailed Description

Phone Alert Status Service init stucture. This contains all option and data needed for initialization of the service.

Definition at line 156 of file pass.h.

## Member Data Documentation

## ◆ alert_status

uint8_t pass_init_t::alert_status

Initial alert status.

Definition at line 160 of file pass.h.

## ◆ char_mask

uint16_t pass_init_t::char_mask

Initial mask of supported characteristics, and configured with Characteristics Mask.

Definition at line 159 of file pass.h.

## ◆ evt_handler

pass_evt_handler_t pass_init_t::evt_handler

Phone Alert Status Service event handler.

Definition at line 158 of file pass.h.

## ◆ ringer_setting

uint8_t pass_init_t::ringer_setting

Initial ringer setting.

Definition at line 161 of file pass.h.

The documentation for this struct was generated from the following file:

- pass.h