ble_l2cap.h
Go to the documentation of this file.
1 /**
2 ****************************************************************************************
3 *
4 * @file ble_l2cap.h
5 *
6 * @brief BLE L2CAP API
7 *
8 ****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE
40 * @{
41 */
42
43 /**
44 @addtogroup BLE_L2CAP Logical Link Control and Adaptation Protocol (L2CAP)
45 @{
46 @brief Definitions and prototypes for the L2CAP interface.
47 */
48
49 #ifndef __BLE_L2CAP_H__
50 #define __BLE_L2CAP_H__
51
52 #include "ble_error.h"
53 #include "gr55xx_sys_cfg.h"
54 #include <stdint.h>
55 #include <stdbool.h>
56
57 /**@addtogroup BLE_L2CAP_ENUMERATIONS Enumerations
58 * @{ */
59
60 /**@brief LE credit based disconnection reasons. */
61 typedef enum
62 {
63 BLE_L2CAP_REMOTE_USER_TERM_CON = 0x00, /**< Remote user terminates the connection. */
64 BLE_L2CAP_LOCAL_USER_TERM_CON = 0x01, /**< Local user terminates the connection. */
65 } ble_l2cap_lecb_disconn_reason_t;
66
67 /** @} */
68
69 /** @addtogroup BLE_L2CAP_STRUCTURES Structures
70 * @{ */
71 /** @brief The parameter of LE credit based connection request packet sending.
72 * @note The le_psm should be registered by the peer device, otherwise the peer device will reject this request with result of LE_PSM not supported.
73 * @note The local_cid should be 0x0040-0x007F. If the local_cid is set to 0, the stack will assign it dynamically.
74 * @note The local_credit is required to be sure that at least one SDU can be received, otherwise the stack will use the default value: (MTU + MPS + 1) /MPS + 1.
75 * @note The MTU range is [23~max_mtu].
76 * @note The MPS range is [23~max_mps].
77 * @note About max_mtu and max_mps config, please see @ref ble_gap_l2cap_params_set.
78 */
79 typedef struct
80 {
81 uint16_t le_psm; /**< The le_psm number. */
82 uint16_t local_cid; /**< The local CID. */
83 uint16_t local_credits; /**< The local credits indicate the number of LE-frames that the peer device can send to the L2CAP layer entity sending the LE Credit Based Connection Request. */
84 uint16_t mtu; /**< The MTU field specifies the maximum SDU size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request can receive on this channel. */
85 uint16_t mps; /**< The MPS field specifies the maximum payload size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request is capable of receiving on this channel. */
86 } ble_l2cap_lecb_conn_req_t;
87
88 /** @brief LE credit based connection confirm parameter.
89 * @note The accept flag indicates whether the App accepts the LE Credit Based connection request.
90 * @note The peer_cid represents the channel endpoint on the peer device.
91 * @note The local_cid should be 0x0040-0x007F. If the local_cid is set to 0, the stack will assign it dynamically.
92 * @note The local_credits required to be sure that at least one SDU can be received, otherwise the stack will use the default value: (MTU + MPS + 1) /MPS + 1.
93 * @note The MTU range is [23~max_mtu].
94 * @note The MPS range is [23~max_mps].
95 * @note About the max_mtu and max_mps config, please see @ref ble_gap_l2cap_params_set.
96 */
97 typedef struct
98 {
99 bool accept; /**< Whether to accept the connection request. */
100 uint16_t peer_cid; /**< It represents the channel endpoint on the device sending the request and receiving the response. */
101 uint16_t local_cid; /**< Local CID. */
102 uint16_t local_credits; /**< It indicates the number of LE-frames that the peer device can send to the L2CAP layer entity sending the LE Credit Based Connection Respone. */
103 uint16_t mtu; /**< The MTU field specifies the maximum SDU size (in octets) that the L2CAP layer entity sending
104 the LE Credit Based Connection Request can receive on this channel. */
105 uint16_t mps; /**< The MPS field specifies the maximum payload size (in octets) that the L2CAP layer entity sending
106 the LE Credit Based Connection Request is capable of receiving on this channel. */
107 } ble_l2cap_lecb_cfm_conn_t;
108
109 /** @brief LE flow control credit packet parameter. */
110 typedef struct
111 {
112 uint16_t local_cid; /**< The local source channel ID. */
113 uint16_t credits; /**< Number of credits that the receiving device can increment. */
114 } ble_l2cap_lecb_add_credits_t;
115
116 /** @brief SDU packet parameter.
117 * @note The length should be less than peer_mtu when sending sdu packet.
118 * @note The credits is 0 if this packet is being sent, or it represents the number of credits consumed by this sdu if this packet is received.
119 * @note When the application receives a sdu, it should firstly copy this sdu packet before handling it, because the stack will free it after invoking the callback function.
120 * @note Similarly, the application should free the packet if it is malloced after invoking the function to send sdu packet.
121 */
122 typedef struct
123 {
124 uint16_t cid; /**< The local source channel. */
125 uint16_t credits; /**< The credits is 0 if this packet is being sent, otherwise it represents the number of credits consumed by the sdu. */
126 uint16_t length; /**< The lenght of data. */
127 uint8_t *data; /**< The data of this sdu packet. */
128 } ble_l2cap_lecb_sdu_t;
129
130 /** @brief L2cap Connect Request event for @ref BLE_L2CAP_EVT_CONN_REQ. */
131 typedef struct
132 {
133 uint16_t le_psm; /**< Le_psm number that should be registered by local device. */
134 uint16_t peer_cid; /**< It represents the channel endpoint on the device sending the request and receiving the response. */
135 uint16_t peer_mtu; /**< It indicates the maximum SDU size (in octets) that the L2CAP layer entity sending the LE Credit
136 Based Connection Request can receive on this channel. */
137 uint16_t peer_mps; /**< It indicates the maximum payload size (in octets) that the L2CAP layer entity sending the LE Credit
138 Based Connection Request is capable of receiving on this channe. */
139 } ble_l2cap_evt_conn_req_t;
140
141 /** @brief L2cap Connected Indicate event for @ref BLE_L2CAP_EVT_CONN_IND. */
142 typedef struct
143 {
144 uint16_t le_psm; /**< Le_psm number. */
145 uint16_t local_cid; /**< The local source channel ID. */
146 uint16_t local_credits; /**< It indicates the number of LE-frames that the local device can receive. */
147 uint16_t peer_credits; /**< It indicates the number of LE-frames that the peer device can receive. */
148 uint16_t peer_mtu; /**< It indicates the maximum SDU size (in octets) that the L2CAP layer entity sending the LE Credit
149 Based Connection Request can receive on this channel. */
150 uint16_t peer_mps; /**< It indicates the maximum payload size (in octets) that the L2CAP layer entity sending the LE Credit
151 Based Connection Request is capable of receiving on this channe. */
152 } ble_l2cap_evt_conn_ind_t;
153
154 /** @brief L2cap Credits Add Indicate event for @ref BLE_L2CAP_EVT_ADD_CREDITS_IND. */
155 typedef struct
156 {
157 uint16_t local_cid; /**< The local source channel ID. */
158 uint16_t peer_added_credits; /**< Represent number of credits the receiving device can increment. */
159 } ble_l2cap_evt_add_credits_ind_t;
160
161 /** @brief L2cap disconnect event for @ref BLE_L2CAP_EVT_DISCONNECTED. */
162 typedef struct
163 {
164 uint16_t local_cid; /**< The local source channel ID. */
165 ble_l2cap_lecb_disconn_reason_t reason; /**< The reason for disconnection, see @ref ble_l2cap_lecb_disconn_reason_t . */
166 } ble_l2cap_evt_disconnect_t;
167
168 /**@brief L2cap SDU Receive event for @ref BLE_L2CAP_EVT_SDU_RECV. */
169 typedef struct
170 {
171 uint16_t cid; /**< The local source channel. */
172 uint16_t credits; /**< The credits is 0 if this packet is being sent, otherwise it represents the number of credits consumed by the sdu. */
173 uint16_t length; /**< The lenght of data. */
174 uint8_t *data; /**< The data of this sdu packet. */
175 } ble_l2cap_evt_sdu_recv_t;
176
177 /**@brief L2cap SDU Send event for @ref BLE_L2CAP_EVT_SDU_SEND. */
178 typedef struct
179 {
180 uint16_t cid; /**< Channel ID that is the local CID. */
181 uint16_t credits; /**< Number of peer credit used. */
182 }ble_l2cap_evt_sdu_send_t;
183
184 /**@brief L2cap Credits Add Completed event for @ref BLE_GATTC_EVT_NTF_IND. */
185 typedef struct
186 {
187 uint16_t local_cid; /**< Channel ID that is the local CID. */
188 }ble_l2cap_evt_add_credits_cplt_t;
189
190 /**@brief BLE L2cap event structure. */
191 typedef struct
192 {
193 uint8_t index; /**< Index of connection or advertising. */
194 union
195 {
196 ble_l2cap_evt_conn_req_t conn_req; /**< L2cap Connect Request event. */
197 ble_l2cap_evt_conn_ind_t conn_ind; /**< L2cap Connected Indicate event. */
198 ble_l2cap_evt_add_credits_ind_t add_credits_ind; /**< L2cap Credits Add Indicate event. */
199 ble_l2cap_evt_disconnect_t disconnected; /**< L2cap Disconnected event. */
200 ble_l2cap_evt_sdu_recv_t sdu_recv; /**< L2cap SDU Receive event. */
201 ble_l2cap_evt_sdu_send_t sdu_send; /**< L2cap SDU Send event. */
202 ble_l2cap_evt_add_credits_cplt_t add_credits_cplt; /**< L2cap Credits Add Completed event. */
203 } params; /**< Event Parameters. */
204 } ble_l2cap_evt_t;
205 /** @} */
206
207 /** @addtogroup BLE_L2CAP_FUNCTIONS Functions
208 * @{ */
209 /**
210 ****************************************************************************************
211 * @brief Create the LE credit based connection.
212 *
213 * @param[in] conn_idx: ACL connection index. The first ACL connection index is 0, and the index will be increased one by one.
214 * @param[in] p_conn_req: Pointer to the LE Credit Based Connection Request structure.
215 *
216 * @retval ::SDK_SUCCESS: The LE Credit Based connection request is successfully set to the BLE stack.
217 * @retval ::SDK_ERR_POINTER_NULL: Invalid pointer supplied.
218 * @retval ::SDK_ERR_INVALID_CONN_IDX: Invalid connection index supplied.
219 * @retval ::SDK_ERR_NO_RESOURCES: Not enough resources.
220 ****************************************************************************************
221 */
222 uint16_t ble_l2cap_lecb_conn_create(uint8_t conn_idx, const ble_l2cap_lecb_conn_req_t *p_conn_req);
223
224 /**
225 ****************************************************************************************
226 * @brief Confirm the LE credit based connection after receiving the connection request packet from the peer device.
227 *
228 * @param[in] conn_idx: ACL connection index. The first ACL connection index is 0 and the index will be increased one by one.
229 * @param[in] p_cfm_conn: Pointer to the LE Credit Based Connection Confirm structure.
230 *
231 * @retval ::SDK_SUCCESS: The LE Credit Based connection confirmation is successfully set to the BLE stack.
232 * @retval ::SDK_ERR_POINTER_NULL: Invalid pointer supplied.
233 * @retval ::SDK_ERR_INVALID_CONN_IDX: Invalid connection index supplied.
234 * @retval ::SDK_ERR_INVALID_PARAM: Invalid parameter supplied.
235 * @retval ::SDK_ERR_NO_RESOURCES: Not enough resources.
236 ****************************************************************************************
237 */
238 uint16_t ble_l2cap_lecb_conn_cfm(uint8_t conn_idx, const ble_l2cap_lecb_cfm_conn_t *p_cfm_conn);
239
240 /**
241 ****************************************************************************************
242 * @brief Disconnect the LE credit based connection.
243 *
244 * @param[in] conn_idx: ACL connection index. The first ACL connection index is 0 and the index will be increased one by one.
245 * @param[in] local_cid: The local source channel ID.
246 *
247 * @retval ::SDK_SUCCESS: LE Credit Based disconnection request is successfully set to the BLE stack.
248 * @retval ::SDK_ERR_INVALID_CONN_IDX: Invalid connection index supplied.
249 * @retval ::SDK_ERR_NO_RESOURCES: Not enough resources.
250 ****************************************************************************************
251 */
252 uint16_t ble_l2cap_lecb_disconnect(uint8_t conn_idx, uint16_t local_cid);
253
254 /**
255 ****************************************************************************************
256 * @brief Send a LE Flow Control Credit packet when the device is capable of receiving additional LE-frames (for example after the device has processed the sdu).
257 *
258 * @param[in] conn_idx: ACL connection index, the first ACL connection index is 0, and increased one by one.
259 * @param[in] p_add_credits: Pointer to the LE Flow Control Credit structure.
260 *
261 * @retval ::SDK_SUCCESS: LE Flow Control Credit packet is successfully set to the BLE stack.
262 * @retval ::SDK_ERR_POINTER_NULL: Invalid pointer supplied.
263 * @retval ::SDK_ERR_INVALID_CONN_IDX: Invalid connection index supplied.
264 * @retval ::SDK_ERR_NO_RESOURCES: Not enough resources.
265 ****************************************************************************************
266 */
267 uint16_t ble_l2cap_lecb_credits_add(uint8_t conn_idx, const ble_l2cap_lecb_add_credits_t *p_add_credits);
268
269 /**
270 ****************************************************************************************
271 * @brief Send an SDU packet to the peer device.
272 *
273 * @param[in] conn_idx: ACL connection index. The first ACL connection index is 0 and the index will be increased one by one.
274 * @param[in] p_sdu: Pointer to the sdu packet structure.
275 *
276 * @retval ::SDK_SUCCESS: The sdu packet is successfully set to the BLE stack.
277 * @retval ::SDK_ERR_POINTER_NULL: Invalid pointer supplied.
278 * @retval ::SDK_ERR_INVALID_CONN_IDX: Invalid connection index supplied.
279 * @retval ::SDK_ERR_NO_RESOURCES: Not enough resources.
280 ****************************************************************************************
281 */
282 uint16_t ble_l2cap_lecb_sdu_send(uint8_t conn_idx, const ble_l2cap_lecb_sdu_t *p_sdu);
283
284 /**
285 ****************************************************************************************
286 * @brief Register PSM.
287 *
288 * @param[in] le_psm: The le_psm number.
289 *
290 * @retval ::SDK_SUCCESS: The callback is successfully registered to the BLE stack.
291 * @retval ::SDK_ERR_INVALID_PARAM: Invalid parameter supplied.
292 * @retval ::SDK_ERR_INVALID_PSM_EXCEEDED_MAX_PSM_NUM: The maximum PSM number limit is exceeded.
293 ****************************************************************************************
294 */
295 uint16_t ble_l2cap_lecb_psm_register(uint16_t le_psm);
296 /** @} */
297
298 #endif
299
300 /**
301 @}
302 */
303 /** @} */
ble_l2cap_evt_conn_req_t::peer_cid
uint16_t peer_cid
Definition: ble_l2cap.h:134
ble_l2cap_evt_conn_req_t::peer_mtu
uint16_t peer_mtu
Definition: ble_l2cap.h:135
ble_l2cap_evt_add_credits_ind_t::peer_added_credits
uint16_t peer_added_credits
Definition: ble_l2cap.h:158
ble_l2cap_evt_t::index
uint8_t index
Definition: ble_l2cap.h:193
ble_l2cap_lecb_cfm_conn_t::mtu
uint16_t mtu
Definition: ble_l2cap.h:103
ble_l2cap_lecb_conn_req_t
The parameter of LE credit based connection request packet sending.
Definition: ble_l2cap.h:80
ble_l2cap_evt_conn_req_t
L2cap Connect Request event for BLE_L2CAP_EVT_CONN_REQ.
Definition: ble_l2cap.h:132
ble_l2cap_evt_conn_ind_t::peer_mtu
uint16_t peer_mtu
Definition: ble_l2cap.h:148
ble_l2cap_lecb_conn_req_t::le_psm
uint16_t le_psm
Definition: ble_l2cap.h:81
ble_l2cap_lecb_add_credits_t
LE flow control credit packet parameter.
Definition: ble_l2cap.h:111
ble_l2cap_evt_add_credits_cplt_t
L2cap Credits Add Completed event for BLE_GATTC_EVT_NTF_IND.
Definition: ble_l2cap.h:186
ble_l2cap_lecb_cfm_conn_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:101
ble_l2cap_evt_conn_ind_t::local_credits
uint16_t local_credits
Definition: ble_l2cap.h:146
BLE_L2CAP_REMOTE_USER_TERM_CON
@ BLE_L2CAP_REMOTE_USER_TERM_CON
Definition: ble_l2cap.h:63
ble_l2cap_lecb_sdu_t::cid
uint16_t cid
Definition: ble_l2cap.h:124
ble_l2cap_evt_sdu_recv_t::length
uint16_t length
Definition: ble_l2cap.h:173
ble_l2cap_lecb_psm_register
uint16_t ble_l2cap_lecb_psm_register(uint16_t le_psm)
Register PSM.
ble_l2cap_evt_conn_req_t::le_psm
uint16_t le_psm
Definition: ble_l2cap.h:133
ble_l2cap_evt_conn_ind_t::peer_credits
uint16_t peer_credits
Definition: ble_l2cap.h:147
ble_l2cap_evt_t::disconnected
ble_l2cap_evt_disconnect_t disconnected
Definition: ble_l2cap.h:199
ble_l2cap_evt_t
BLE L2cap event structure.
Definition: ble_l2cap.h:192
ble_l2cap_evt_add_credits_ind_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:157
ble_l2cap_lecb_sdu_t::length
uint16_t length
Definition: ble_l2cap.h:126
ble_l2cap_lecb_sdu_send
uint16_t ble_l2cap_lecb_sdu_send(uint8_t conn_idx, const ble_l2cap_lecb_sdu_t *p_sdu)
Send an SDU packet to the peer device.
ble_l2cap_lecb_disconnect
uint16_t ble_l2cap_lecb_disconnect(uint8_t conn_idx, uint16_t local_cid)
Disconnect the LE credit based connection.
ble_l2cap_evt_sdu_recv_t::credits
uint16_t credits
Definition: ble_l2cap.h:172
ble_l2cap_evt_conn_ind_t::le_psm
uint16_t le_psm
Definition: ble_l2cap.h:144
ble_l2cap_lecb_conn_req_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:82
gr55xx_sys_cfg.h
Define the chip configuration.
ble_l2cap_lecb_add_credits_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:112
ble_l2cap_evt_t::sdu_send
ble_l2cap_evt_sdu_send_t sdu_send
Definition: ble_l2cap.h:201
BLE_L2CAP_LOCAL_USER_TERM_CON
@ BLE_L2CAP_LOCAL_USER_TERM_CON
Definition: ble_l2cap.h:64
ble_l2cap_lecb_conn_create
uint16_t ble_l2cap_lecb_conn_create(uint8_t conn_idx, const ble_l2cap_lecb_conn_req_t *p_conn_req)
Create the LE credit based connection.
ble_l2cap_evt_conn_ind_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:145
ble_l2cap_evt_t::add_credits_cplt
ble_l2cap_evt_add_credits_cplt_t add_credits_cplt
Definition: ble_l2cap.h:202
ble_l2cap_evt_t::sdu_recv
ble_l2cap_evt_sdu_recv_t sdu_recv
Definition: ble_l2cap.h:200
ble_error.h
File that contains error codes.
ble_l2cap_evt_sdu_send_t
L2cap SDU Send event for BLE_L2CAP_EVT_SDU_SEND.
Definition: ble_l2cap.h:179
ble_l2cap_lecb_add_credits_t::credits
uint16_t credits
Definition: ble_l2cap.h:113
ble_l2cap_evt_sdu_recv_t::cid
uint16_t cid
Definition: ble_l2cap.h:171
ble_l2cap_lecb_disconn_reason_t
ble_l2cap_lecb_disconn_reason_t
LE credit based disconnection reasons.
Definition: ble_l2cap.h:62
ble_l2cap_lecb_cfm_conn_t::accept
bool accept
Definition: ble_l2cap.h:99
ble_l2cap_evt_add_credits_ind_t
L2cap Credits Add Indicate event for BLE_L2CAP_EVT_ADD_CREDITS_IND.
Definition: ble_l2cap.h:156
ble_l2cap_lecb_conn_cfm
uint16_t ble_l2cap_lecb_conn_cfm(uint8_t conn_idx, const ble_l2cap_lecb_cfm_conn_t *p_cfm_conn)
Confirm the LE credit based connection after receiving the connection request packet from the peer de...
ble_l2cap_evt_t::add_credits_ind
ble_l2cap_evt_add_credits_ind_t add_credits_ind
Definition: ble_l2cap.h:198
ble_l2cap_evt_add_credits_cplt_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:187
ble_l2cap_lecb_cfm_conn_t::peer_cid
uint16_t peer_cid
Definition: ble_l2cap.h:100
ble_l2cap_evt_sdu_recv_t::data
uint8_t * data
Definition: ble_l2cap.h:174
ble_l2cap_evt_conn_ind_t
L2cap Connected Indicate event for BLE_L2CAP_EVT_CONN_IND.
Definition: ble_l2cap.h:143
ble_l2cap_lecb_sdu_t
SDU packet parameter.
Definition: ble_l2cap.h:123
ble_l2cap_evt_t::conn_req
ble_l2cap_evt_conn_req_t conn_req
Definition: ble_l2cap.h:196
ble_l2cap_evt_t::conn_ind
ble_l2cap_evt_conn_ind_t conn_ind
Definition: ble_l2cap.h:197
ble_l2cap_lecb_credits_add
uint16_t ble_l2cap_lecb_credits_add(uint8_t conn_idx, const ble_l2cap_lecb_add_credits_t *p_add_credits)
Send a LE Flow Control Credit packet when the device is capable of receiving additional LE-frames (fo...
ble_l2cap_lecb_cfm_conn_t::local_credits
uint16_t local_credits
Definition: ble_l2cap.h:102
ble_l2cap_lecb_sdu_t::credits
uint16_t credits
Definition: ble_l2cap.h:125
ble_l2cap_lecb_conn_req_t::local_credits
uint16_t local_credits
Definition: ble_l2cap.h:83
ble_l2cap_lecb_cfm_conn_t::mps
uint16_t mps
Definition: ble_l2cap.h:105
ble_l2cap_evt_sdu_recv_t
L2cap SDU Receive event for BLE_L2CAP_EVT_SDU_RECV.
Definition: ble_l2cap.h:170
ble_l2cap_lecb_cfm_conn_t
LE credit based connection confirm parameter.
Definition: ble_l2cap.h:98
ble_l2cap_lecb_conn_req_t::mtu
uint16_t mtu
Definition: ble_l2cap.h:84
ble_l2cap_evt_disconnect_t
L2cap disconnect event for BLE_L2CAP_EVT_DISCONNECTED.
Definition: ble_l2cap.h:163
ble_l2cap_lecb_conn_req_t::mps
uint16_t mps
Definition: ble_l2cap.h:85
ble_l2cap_evt_conn_ind_t::peer_mps
uint16_t peer_mps
Definition: ble_l2cap.h:150
ble_l2cap_evt_disconnect_t::reason
ble_l2cap_lecb_disconn_reason_t reason
Definition: ble_l2cap.h:165
ble_l2cap_evt_disconnect_t::local_cid
uint16_t local_cid
Definition: ble_l2cap.h:164
ble_l2cap_evt_sdu_send_t::cid
uint16_t cid
Definition: ble_l2cap.h:180
ble_l2cap_evt_sdu_send_t::credits
uint16_t credits
Definition: ble_l2cap.h:181
ble_l2cap_lecb_sdu_t::data
uint8_t * data
Definition: ble_l2cap.h:127
ble_l2cap_evt_conn_req_t::peer_mps
uint16_t peer_mps
Definition: ble_l2cap.h:137