Here is a list of all file members with links to the files they belong to:

### - m -

- MEAS_PACKET_FIRST : bcs.h
- MEAS_PACKET_SUB : bcs.h
- mem_check_proc_t : gr55xx_pwr.h
- MEM_POWER_AUTO_MODE : platform_sdk.h
- MEM_POWER_FULL_MODE : platform_sdk.h
- mem_power_t : platform_sdk.h
- mem_pwr_mgmt_full_power_set() : platform_sdk.h
- mem_pwr_mgmt_init() : platform_sdk.h
- mem_pwr_mgmt_mode_set_from() : platform_sdk.h
- MIRROR_16M : platform_sdk.h
- MIRROR_24M : platform_sdk.h
- MIRROR_32M : platform_sdk.h
- MIRROR_48M : platform_sdk.h
- MIRROR_64M : platform_sdk.h
- MIRROR_XO16M : platform_sdk.h
- MLMR_C_CONNECTION_MAX : mlmr_c.h
- mlmr_c_disc_srvc_start() : mlmr_c.h
- MLMR_C_EVT_DISCOVERY_COMPLETE : mlmr_c.h
- MLMR_C_EVT_DISCOVERY_FAIL : mlmr_c.h
- MLMR_C_EVT_FLOW_CTRL_NTF_SET_SUCCESS : mlmr_c.h
- mlmr_c_evt_handler_t : mlmr_c.h
- MLMR_C_EVT_INVALID : mlmr_c.h
- MLMR_C_EVT_PEER_DATA_RECEIVE : mlmr_c.h
- MLMR_C_EVT_RX_FLOW_UPDATE_CPLT : mlmr_c.h
- MLMR_C_EVT_TX_CPLT : mlmr_c.h
- MLMR_C_EVT_TX_FLOW_OFF : mlmr_c.h
- MLMR_C_EVT_TX_FLOW_ON : mlmr_c.h
- MLMR_C_EVT_TX_NTF_SET_SUCCESS : mlmr_c.h
- mlmr_c_evt_type_t : mlmr_c.h
- MLMR_C_EVT_WRITE_OP_ERR : mlmr_c.h
- mlmr_c_flow_ctrl_notify_set() : mlmr_c.h
- mlmr_c_flow_ctrl_state : mlmr_c.h
- MLMR_C_FLOW_CTRL_STATE_OFF : mlmr_c.h
- MLMR_C_FLOW_CTRL_STATE_ON : mlmr_c.h
- mlmr_c_flow_ctrl_state_t : mlmr_c.h
- MLMR_C_FLOW_CTRL_UUID : mlmr_c.h
- MLMR_C_RX_CHAR_UUID : mlmr_c.h
- mlmr_c_rx_flow_ctrl_set() : mlmr_c.h
- MLMR_C_SVC_UUID : mlmr_c.h
- MLMR_C_TX_CHAR_UUID : mlmr_c.h
- mlmr_c_tx_data_send() : mlmr_c.h
- mlmr_c_tx_notify_set() : mlmr_c.h
- mlmr_client_init() : mlmr_c.h
- MLMR_CONNECTION_MAX : mlmr.h
- MLMR_EVT_FLOW_CTRL_DISABLE : mlmr.h
- MLMR_EVT_FLOW_CTRL_ENABLE : mlmr.h
- mlmr_evt_handler_t : mlmr.h
- MLMR_EVT_INVALID : mlmr.h
- MLMR_EVT_RX_DATA_RECEIVED : mlmr.h
- MLMR_EVT_TX_DATA_SENT : mlmr.h
- MLMR_EVT_TX_FLOW_OFF : mlmr.h
- MLMR_EVT_TX_FLOW_ON : mlmr.h
- MLMR_EVT_TX_PORT_CLOSED : mlmr.h
- MLMR_EVT_TX_PORT_OPENED : mlmr.h
- mlmr_evt_type_t : mlmr.h
- MLMR_FLOW_CTRL_LEN : mlmr.h
- mlmr_flow_ctrl_state : mlmr.h
- MLMR_FLOW_CTRL_STATE_OFF : mlmr.h
- MLMR_FLOW_CTRL_STATE_ON : mlmr.h
- mlmr_flow_ctrl_state_t : mlmr.h
- MLMR_MAX_DATA_LEN : mlmr.h
- mlmr_rx_flow_ctrl_set() : mlmr.h
- mlmr_service_init() : mlmr.h
- MLMR_SERVICE_UUID : mlmr.h
- mlmr_tx_data_send() : mlmr.h
- MPU_ACCESS_BUFFERABLE : gr55xx_hal_cortex.h
- MPU_ACCESS_CACHEABLE : gr55xx_hal_cortex.h
- MPU_ACCESS_NOT_BUFFERABLE : gr55xx_hal_cortex.h
- MPU_ACCESS_NOT_CACHEABLE : gr55xx_hal_cortex.h
- MPU_ACCESS_NOT_SHAREABLE : gr55xx_hal_cortex.h
- MPU_ACCESS_SHAREABLE : gr55xx_hal_cortex.h
- MPU_HARDFAULT_NMI : gr55xx_hal_cortex.h
- MPU_HFNMI_PRIVDEF : gr55xx_hal_cortex.h
- MPU_HFNMI_PRIVDEF_NONE : gr55xx_hal_cortex.h
- MPU_INSTRUCTION_ACCESS_DISABLE : gr55xx_hal_cortex.h
- MPU_INSTRUCTION_ACCESS_ENABLE : gr55xx_hal_cortex.h
- MPU_PRIVILEGED_DEFAULT : gr55xx_hal_cortex.h
- MPU_REGION_DISABLE : gr55xx_hal_cortex.h
- MPU_REGION_ENABLE : gr55xx_hal_cortex.h
- MPU_REGION_FULL_ACCESS : gr55xx_hal_cortex.h
- mpu_region_init_t : gr55xx_hal_cortex.h
- MPU_REGION_NO_ACCESS : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER0 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER1 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER2 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER3 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER4 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER5 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER6 : gr55xx_hal_cortex.h
- MPU_REGION_NUMBER7 : gr55xx_hal_cortex.h
- MPU_REGION_PRIV_RO : gr55xx_hal_cortex.h
- MPU_REGION_PRIV_RO_URO : gr55xx_hal_cortex.h
- MPU_REGION_PRIV_RW : gr55xx_hal_cortex.h
- MPU_REGION_PRIV_RW_URO : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_128B : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_128KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_128MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_16KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_16MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_1GB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_1KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_1MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_256B : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_256KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_256MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_2GB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_2KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_2MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_32B : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_32KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_32MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_4GB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_4KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_4MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_512B : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_512KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_512MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_64B : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_64KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_64MB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_8KB : gr55xx_hal_cortex.h
- MPU_REGION_SIZE_8MB : gr55xx_hal_cortex.h
- MPU_TEX_LEVEL0 : gr55xx_hal_cortex.h
- MPU_TEX_LEVEL1 : gr55xx_hal_cortex.h
- MPU_TEX_LEVEL2 : gr55xx_hal_cortex.h
- msg_tab : patch_tab.h
- MSIO_DEFAULT_CONFIG : gr55xx_hal_msio.h
- MSIO_DIRECTION_INOUT : gr55xx_hal_msio.h
- MSIO_DIRECTION_INPUT : gr55xx_hal_msio.h
- MSIO_DIRECTION_NONE : gr55xx_hal_msio.h
- MSIO_DIRECTION_OUTPUT : gr55xx_hal_msio.h
- msio_init_t : gr55xx_hal_msio.h
- MSIO_MODE_ANALOG : gr55xx_hal_msio.h
- MSIO_MODE_DIGITAL : gr55xx_hal_msio.h
- MSIO_MUX_0 : gr55xx_hal_msio_ex.h
- MSIO_MUX_1 : gr55xx_hal_msio_ex.h
- MSIO_MUX_2 : gr55xx_hal_msio_ex.h
- MSIO_MUX_3 : gr55xx_hal_msio_ex.h
- MSIO_MUX_4 : gr55xx_hal_msio_ex.h
- MSIO_MUX_5 : gr55xx_hal_msio_ex.h
- MSIO_MUX_6 : gr55xx_hal_msio_ex.h
- MSIO_MUX_7 : gr55xx_hal_msio_ex.h
- MSIO_NOPULL : gr55xx_hal_msio.h
- msio_pad_t : gr55xx_ll_msio.h
- MSIO_PIN0_MUX_I2C0_SCL : gr55xx_hal_msio_ex.h
- MSIO_PIN0_MUX_I2C1_SCL : gr55xx_hal_msio_ex.h
- MSIO_PIN0_MUX_PWM0_A : gr55xx_hal_msio_ex.h
- MSIO_PIN0_MUX_UART0_TX : gr55xx_hal_msio_ex.h
- MSIO_PIN0_MUX_UART1_TX : gr55xx_hal_msio_ex.h
- MSIO_PIN1_MUX_I2C0_SDA : gr55xx_hal_msio_ex.h
- MSIO_PIN1_MUX_I2C1_SDA : gr55xx_hal_msio_ex.h
- MSIO_PIN1_MUX_PWM0_B : gr55xx_hal_msio_ex.h
- MSIO_PIN1_MUX_UART0_RX : gr55xx_hal_msio_ex.h
- MSIO_PIN1_MUX_UART1_RX : gr55xx_hal_msio_ex.h
- MSIO_PIN2_MUX_PWM0_C : gr55xx_hal_msio_ex.h
- MSIO_PIN3_MUX_I2C0_SCL : gr55xx_hal_msio_ex.h
- MSIO_PIN3_MUX_I2C1_SCL : gr55xx_hal_msio_ex.h
- MSIO_PIN3_MUX_PWM1_A : gr55xx_hal_msio_ex.h
- MSIO_PIN3_MUX_UART0_RTS : gr55xx_hal_msio_ex.h
- MSIO_PIN3_MUX_UART1_RTS : gr55xx_hal_msio_ex.h
- MSIO_PIN4_MUX_I2C0_SDA : gr55xx_hal_msio_ex.h
- MSIO_PIN4_MUX_I2C1_SDA : gr55xx_hal_msio_ex.h
- MSIO_PIN4_MUX_PWM1_B : gr55xx_hal_msio_ex.h
- MSIO_PIN4_MUX_UART0_CTS : gr55xx_hal_msio_ex.h
- MSIO_PIN4_MUX_UART1_CTS : gr55xx_hal_msio_ex.h
- MSIO_PIN_0 : gr55xx_hal_msio.h
- MSIO_PIN_1 : gr55xx_hal_msio.h
- MSIO_PIN_2 : gr55xx_hal_msio.h
- MSIO_PIN_3 : gr55xx_hal_msio.h
- MSIO_PIN_4 : gr55xx_hal_msio.h
- MSIO_PIN_ALL : gr55xx_hal_msio.h
- MSIO_PIN_MASK : gr55xx_hal_msio.h
- MSIO_PIN_MUX_GPIO : gr55xx_hal_msio_ex.h
- MSIO_PIN_RESET : gr55xx_hal_msio.h
- MSIO_PIN_SET : gr55xx_hal_msio.h
- msio_pin_state_t : gr55xx_hal_msio.h
- MSIO_PULLDOWN : gr55xx_hal_msio.h
- MSIO_PULLUP : gr55xx_hal_msio.h
- MSIOA : gr55xx_ll_msio.h
- MUTEX_NO_WAIT : app_rtos_cfg.h
- mutex_t : app_rtos_cfg.h
- MUTEX_WAIT_FOREVER : app_rtos_cfg.h