Public Attributes | List of all members
ble_gap_lepsm_register_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

LE Protocol/Service Multiplexer information. More...

`#include <ble_gapm.h>`

## Public Attributes
uint16_t | le_psm
ble_gap_sec_lvl_type_t | sec_lvl
bool | mks_flag

## Detailed Description

LE Protocol/Service Multiplexer information.

Definition at line 727 of file ble_gapm.h.

## Member Data Documentation

## ◆ le_psm

uint16_t ble_gap_lepsm_register_t::le_psm

LE Protocol/Service Multiplexer (range: 1 to 255), PSMs should be odd.

Definition at line 729 of file ble_gapm.h.

## ◆ mks_flag

bool ble_gap_lepsm_register_t::mks_flag

Whether to use maximum-size key (16 bytes) or not.

Definition at line 731 of file ble_gapm.h.

## ◆ sec_lvl

ble_gap_sec_lvl_type_t ble_gap_lepsm_register_t::sec_lvl

Security level requirement, see ble_gap_sec_lvl_type_t.

Definition at line 730 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h