Macros
Defines
BLE Services » OTA Service (OTAS)

## Macros
#define | OTAS_CONNECTION_MAX 10
#define | OTAS_MAX_DATA_LEN 244
#define | OTAS_VERSION 0x02
#define | BLE_UUID_OTA_SERVICE

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_UUID_OTA_SERVICE

#define BLE_UUID_OTA_SERVICE

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x04, 0xED, 0xA6

The UUID of OTA Service for setting advertising data.

Definition at line 78 of file otas.h.

## ◆ OTAS_CONNECTION_MAX

#define OTAS_CONNECTION_MAX 10

Maximum number of OTA Service connections.

Definition at line 74 of file otas.h.

## ◆ OTAS_MAX_DATA_LEN

#define OTAS_MAX_DATA_LEN 244

Maximum length of OTAS characteristic.

Definition at line 75 of file otas.h.

## ◆ OTAS_VERSION

#define OTAS_VERSION 0x02

The OTA VERSION.

Definition at line 76 of file otas.h.