Modules | Macros
AON_GPIO Exported Constants
Peripheral Driver » HAL Driver » AON_GPIO » Defines

## Modules
| AON_GPIO pins
| AON_GPIO mode
| AON_GPIO Configuration Mode Elements values convention: 0x000000YX.
| AON_GPIO pull
| AON_GPIO Pull-Up or Pull-Down activation.

## Macros
#define | AON_GPIO_DEFAULT_CONFIG
| AON_GPIO_default_config initStruct default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ AON_GPIO_DEFAULT_CONFIG

#define AON_GPIO_DEFAULT_CONFIG

Value:
{ \
.pin = AON_GPIO_PIN_ALL, \
.mode = AON_GPIO_MODE_INPUT, \
.pull = AON_GPIO_PULLDOWN, \
.mux = AON_GPIO_MUX_7, \
}

AON_GPIO_default_config initStruct default configuartion.

Definition at line 179 of file gr55xx_hal_aon_gpio.h.

AON_GPIO_MODE_INPUT
#define AON_GPIO_MODE_INPUT
Definition: gr55xx_hal_aon_gpio.h:157
AON_GPIO_MUX_7
#define AON_GPIO_MUX_7
Definition: gr55xx_hal_aon_gpio_ex.h:85
AON_GPIO_PULLDOWN
#define AON_GPIO_PULLDOWN
Definition: gr55xx_hal_aon_gpio.h:173
AON_GPIO_PIN_ALL
#define AON_GPIO_PIN_ALL
Definition: gr55xx_hal_aon_gpio.h:145