Enumerations
Measurement Flag Bits
BLE Services » Body Composition Service (BCS) » Enumerations

## Enumerations
enum | bcs_meas_flag_bits { BCS_MEAS_FLAG_UNIT_SI = 0x0000, BCS_MEAS_FLAG_UNIT_IMPERIAL = 0x0001, BCS_MEAS_FLAG_DATE_TIME_PRESENT = 0x0002, BCS_MEAS_FLAG_USER_ID_PRESENT = 0x0004, BCS_MEAS_FLAG_BASAL_METABOLISM = 0x0008, BCS_MEAS_FLAG_MUSCLE_PERCENTAGE = 0x0010, BCS_MEAS_FLAG_MUSCLE_MASS = 0x0020, BCS_MEAS_FLAG_FAT_FREE_MASS = 0x0040, BCS_MEAS_FLAG_SOFT_LEAN_MASS = 0x0080, BCS_MEAS_FLAG_BODY_WATER_MASS = 0x0100, BCS_MEAS_FLAG_IMPEDANCE = 0x0200, BCS_MEAS_FLAG_WEIGHT = 0x0400, BCS_MEAS_FLAG_HEIGHT = 0x0800, BCS_MEAS_FLAG_MUTI_PACKET = 0x1000 }
| Body Composition Measurement Flags. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ bcs_meas_flag_bits

enum bcs_meas_flag_bits

Body Composition Measurement Flags.

Enumerator
BCS_MEAS_FLAG_UNIT_SI | Flag bit for SI Measurement Units Present.
BCS_MEAS_FLAG_UNIT_IMPERIAL | Flag bit for Imperial Measurement Units Present.
BCS_MEAS_FLAG_DATE_TIME_PRESENT | Flag bit for Time Stamp Present.
BCS_MEAS_FLAG_USER_ID_PRESENT | Flag bit for User ID Present.
BCS_MEAS_FLAG_BASAL_METABOLISM | Flag bit for Basal Metabolism Present.
BCS_MEAS_FLAG_MUSCLE_PERCENTAGE | Flag bit for Muscle Percentage Present.
BCS_MEAS_FLAG_MUSCLE_MASS | Flag bit for Muscle Mass Present.
BCS_MEAS_FLAG_FAT_FREE_MASS | Flag bit for Fat Free Mass Present.
BCS_MEAS_FLAG_SOFT_LEAN_MASS | Flag bit for Soft Lean Mass Present.
BCS_MEAS_FLAG_BODY_WATER_MASS | Flag bit for Body Water Mass Present.
BCS_MEAS_FLAG_IMPEDANCE | Flag bit for Impedance Present.
BCS_MEAS_FLAG_WEIGHT | Flag bit for Weight Present.
BCS_MEAS_FLAG_HEIGHT | Flag bit for Height Present.
BCS_MEAS_FLAG_MUTI_PACKET | Flag bit for Multiple Packet Measurement Present.

Definition at line 119 of file bcs.h.