Macros
QSPI Address Size
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_ADDRSIZE_0BIT 0x00000000UL
#define | LL_SSI_ADDRSIZE_4BIT (1UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_8BIT (2UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_12BIT (3UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_16BIT (4UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_20BIT (5UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_24BIT (6UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_28BIT (7UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_32BIT (8UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_36BIT (9UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_40BIT (10UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_44BIT (11UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_48BIT (12UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_52BIT (13UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_56BIT (14UL << SSI_SCTRL0_ADDRL_Pos)
#define | LL_SSI_ADDRSIZE_60BIT (15UL << SSI_SCTRL0_ADDRL_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_ADDRSIZE_0BIT

#define LL_SSI_ADDRSIZE_0BIT 0x00000000UL

Address length for QSPI transfer: 0 bits

Definition at line 390 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_12BIT

#define LL_SSI_ADDRSIZE_12BIT (3UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 12 bits

Definition at line 393 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_16BIT

#define LL_SSI_ADDRSIZE_16BIT (4UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 16 bits

Definition at line 394 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_20BIT

#define LL_SSI_ADDRSIZE_20BIT (5UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 20 bits

Definition at line 395 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_24BIT

#define LL_SSI_ADDRSIZE_24BIT (6UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 24 bits

Definition at line 396 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_28BIT

#define LL_SSI_ADDRSIZE_28BIT (7UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 28 bits

Definition at line 397 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_32BIT

#define LL_SSI_ADDRSIZE_32BIT (8UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 32 bits

Definition at line 398 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_36BIT

#define LL_SSI_ADDRSIZE_36BIT (9UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 36 bits

Definition at line 399 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_40BIT

#define LL_SSI_ADDRSIZE_40BIT (10UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 40 bits

Definition at line 400 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_44BIT

#define LL_SSI_ADDRSIZE_44BIT (11UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 44 bits

Definition at line 401 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_48BIT

#define LL_SSI_ADDRSIZE_48BIT (12UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 48 bits

Definition at line 402 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_4BIT

#define LL_SSI_ADDRSIZE_4BIT (1UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 4 bits

Definition at line 391 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_52BIT

#define LL_SSI_ADDRSIZE_52BIT (13UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 52 bits

Definition at line 403 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_56BIT

#define LL_SSI_ADDRSIZE_56BIT (14UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 56 bits

Definition at line 404 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_60BIT

#define LL_SSI_ADDRSIZE_60BIT (15UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 60 bits

Definition at line 405 of file gr55xx_ll_spi.h.

## ◆ LL_SSI_ADDRSIZE_8BIT

#define LL_SSI_ADDRSIZE_8BIT (2UL << SSI_SCTRL0_ADDRL_Pos)

Address length for QSPI transfer: 8 bits

Definition at line 392 of file gr55xx_ll_spi.h.