Functions
IRQ Handler and Callbacks
Peripheral Driver » HAL Driver » AES » Functions

IRQ Handler and Callbacks functions. More...

## Functions
void | hal_aes_irq_handler (aes_handle_t *p_aes)
| Handle AES interrupt request. More...
void | hal_aes_done_callback (aes_handle_t *p_aes)
| Encrypt or decrypt Done callback. More...
void | hal_aes_error_callback (aes_handle_t *p_aes)
| AES error callback. More...

## Detailed Description

IRQ Handler and Callbacks functions.

## Function Documentation

## ◆ hal_aes_done_callback()

void hal_aes_done_callback | ( | aes_handle_t * | p_aes | ) |

Encrypt or decrypt Done callback.

Parameters

  [in] | p_aes | Pointer to an AES handle which contains the configuration information for the specified AES module.

## ◆ hal_aes_error_callback()

void hal_aes_error_callback | ( | aes_handle_t * | p_aes | ) |

AES error callback.

Parameters

  [in] | p_aes | Pointer to an AES handle which contains the configuration information for the specified AES module.

## ◆ hal_aes_irq_handler()

void hal_aes_irq_handler | ( | aes_handle_t * | p_aes | ) |

Handle AES interrupt request.

Parameters

  [in] | p_aes | Pointer to an AES handle which contains the configuration information for the specified the specified AES module.