Public Attributes | List of all members
pkc_init_t Struct Reference
Peripheral Driver » HAL Driver » PKC » Structures » PKC Configuration

PKC Init Structure definition. More...

`#include <gr55xx_hal_pkc.h>`

## Public Attributes
ecc_curve_init_t * | p_ecc_curve
uint32_t | data_bits
uint32_t | secure_mode
uint32_t(* | random_func )(void)

## Detailed Description

PKC Init Structure definition.

Definition at line 110 of file gr55xx_hal_pkc.h.

## Member Data Documentation

## ◆ data_bits

uint32_t pkc_init_t::data_bits

Specifies the Data size: 256 ~ 2048 bits

Definition at line 114 of file gr55xx_hal_pkc.h.

## ◆ p_ecc_curve

ecc_curve_init_t* pkc_init_t::p_ecc_curve

Specifies the pointer to elliptic curve description

Definition at line 112 of file gr55xx_hal_pkc.h.

## ◆ random_func

uint32_t(* pkc_init_t::random_func) (void)

Specifies the function to generate random number.

Definition at line 120 of file gr55xx_hal_pkc.h.

## ◆ secure_mode

uint32_t pkc_init_t::secure_mode

Specifies the Secure Mode. It indicates that DPA-resistance software algorithm and hardware measures are applied at a cost of about 35%- 50% performance loss. This parameter can be a value of PKC Secure Mode.

Definition at line 116 of file gr55xx_hal_pkc.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_pkc.h