Modules | Functions
Functions
Peripheral Driver » HAL Driver » SPI

## Modules
| Initialization and de-initialization functions
| Initialization and de-initialization functions.
| IO operation functions
| Data transfer functions.
| Peripheral State and Errors functions
| SPI control functions.
| IRQ Handler and Callbacks
| IRQ Handler and Callbacks functions.

## Functions
void | hal_spi_v2_set_rx_delay (spi_handle_t *p_spi, uint32_t rx_delay)
| set receive sample delay More...

## Detailed Description

## Function Documentation

## ◆ hal_spi_v2_set_rx_delay()

void hal_spi_v2_set_rx_delay | ( | spi_handle_t * | p_spi,
|  | uint32_t | rx_delay
| ) |  |

set receive sample delay

Parameters

  [in] | p_spi | Pointer to an SPI handle which contains the configuration information for the specified SPI module.
  [in] | rx_delay | 0 ~ 7.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.