Macros
Resistor Enable
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Private Macros

## Macros
#define | LL_AON_GPIO_RE_N_Pos AON_PAD_CTL0_GPO_RE_N_Pos
#define | LL_AON_GPIO_RE_N_Msk (0x1U << LL_AON_GPIO_RE_N_Pos)
#define | LL_AON_GPIO_RE_N LL_AON_GPIO_RE_N_Msk

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_RE_N

#define LL_AON_GPIO_RE_N LL_AON_GPIO_RE_N_Msk

Resistor Enable bits

Definition at line 215 of file gr55xx_ll_aon_gpio.h.

## ◆ LL_AON_GPIO_RE_N_Msk

#define LL_AON_GPIO_RE_N_Msk (0x1U << LL_AON_GPIO_RE_N_Pos)

Resistor Enable bits mask

Definition at line 214 of file gr55xx_ll_aon_gpio.h.

## ◆ LL_AON_GPIO_RE_N_Pos

#define LL_AON_GPIO_RE_N_Pos AON_PAD_CTL0_GPO_RE_N_Pos

Resistor Enable bits position

Definition at line 213 of file gr55xx_ll_aon_gpio.h.