### - h -

- HAL_ADC_STATE_BUSY : gr55xx_hal_adc.h
- HAL_ADC_STATE_ERROR : gr55xx_hal_adc.h
- HAL_ADC_STATE_READY : gr55xx_hal_adc.h
- HAL_ADC_STATE_RESET : gr55xx_hal_adc.h
- HAL_AES_STATE_BUSY : gr55xx_hal_aes.h
- HAL_AES_STATE_ERROR : gr55xx_hal_aes.h
- HAL_AES_STATE_READY : gr55xx_hal_aes.h
- HAL_AES_STATE_RESET : gr55xx_hal_aes.h
- HAL_AES_STATE_SUSPENDED : gr55xx_hal_aes.h
- HAL_AES_STATE_TIMEOUT : gr55xx_hal_aes.h
- HAL_BUSY : gr55xx_hal_def.h
- HAL_CALENDAR_STATE_ERROR : gr55xx_hal_calendar.h
- HAL_CALENDAR_STATE_READY : gr55xx_hal_calendar.h
- HAL_CALENDAR_STATE_RESET : gr55xx_hal_calendar.h
- HAL_COMP_STATE_BUSY : gr55xx_hal_comp.h
- HAL_COMP_STATE_ERROR : gr55xx_hal_comp.h
- HAL_COMP_STATE_READY : gr55xx_hal_comp.h
- HAL_COMP_STATE_RESET : gr55xx_hal_comp.h
- HAL_DMA_STATE_BUSY : gr55xx_hal_dma.h
- HAL_DMA_STATE_ERROR : gr55xx_hal_dma.h
- HAL_DMA_STATE_READY : gr55xx_hal_dma.h
- HAL_DMA_STATE_RESET : gr55xx_hal_dma.h
- HAL_DMA_STATE_TIMEOUT : gr55xx_hal_dma.h
- HAL_DMA_XFER_ABORT_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_ALL_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_BLK_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_ERROR_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_TFR_CB_ID : gr55xx_hal_dma.h
- HAL_DUAL_TIMER_STATE_BUSY : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_ERROR : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_READY : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_RESET : gr55xx_hal_dual_tim.h
- HAL_EFUSE_STATE_BUSY : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_ERROR : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_READY : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_RESET : gr55xx_hal_efuse.h
- HAL_ERROR : gr55xx_hal_def.h
- HAL_EXFLASH_ENCRYPTED : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_ERASE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_READ : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_WRITE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_ERROR : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_READY : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_RESET : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_SUSPEND_ERASE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_SUSPEND_WRITE : gr55xx_hal_exflash.h
- HAL_EXFLASH_UNENCRYPTED : gr55xx_hal_exflash.h
- HAL_HMAC_STATE_BUSY : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_ERROR : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_READY : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_RESET : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_SUSPENDED : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_TIMEOUT : gr55xx_hal_hmac.h
- HAL_I2C_MODE_MASTER : gr55xx_hal_i2c.h
- HAL_I2C_MODE_MEM : gr55xx_hal_i2c.h
- HAL_I2C_MODE_NONE : gr55xx_hal_i2c.h
- HAL_I2C_MODE_SLAVE : gr55xx_hal_i2c.h
- HAL_I2C_STATE_ABORT : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_RX : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_RX_LISTEN : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_TX : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_TX_LISTEN : gr55xx_hal_i2c.h
- HAL_I2C_STATE_ERROR : gr55xx_hal_i2c.h
- HAL_I2C_STATE_LISTEN : gr55xx_hal_i2c.h
- HAL_I2C_STATE_READY : gr55xx_hal_i2c.h
- HAL_I2C_STATE_RESET : gr55xx_hal_i2c.h
- HAL_I2C_STATE_TIMEOUT : gr55xx_hal_i2c.h
- HAL_I2S_STATE_ABORT : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_RX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_TX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_TX_RX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_ERROR : gr55xx_hal_i2s.h
- HAL_I2S_STATE_READY : gr55xx_hal_i2s.h
- HAL_I2S_STATE_RESET : gr55xx_hal_i2s.h
- HAL_ISO7816_STATE_ABORT : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_TX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_TX_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_ERROR : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_READY : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_RESET : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_TIMEOUT : gr55xx_hal_iso7816.h
- HAL_LOCKED : gr55xx_hal_def.h
- HAL_OK : gr55xx_hal_def.h
- HAL_PKC_STATE_BUSY : gr55xx_hal_pkc.h
- HAL_PKC_STATE_ERROR : gr55xx_hal_pkc.h
- HAL_PKC_STATE_READY : gr55xx_hal_pkc.h
- HAL_PKC_STATE_RESET : gr55xx_hal_pkc.h
- HAL_PKC_STATE_TIMEOUT : gr55xx_hal_pkc.h
- HAL_PWM_ACTIVE_CHANNEL_A : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_ALL : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_B : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_C : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_CLEARED : gr55xx_hal_pwm.h
- HAL_PWM_STATE_BUSY : gr55xx_hal_pwm.h
- HAL_PWM_STATE_ERROR : gr55xx_hal_pwm.h
- HAL_PWM_STATE_READY : gr55xx_hal_pwm.h
- HAL_PWM_STATE_RESET : gr55xx_hal_pwm.h
- HAL_QSPI_STATE_ABORT : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_INDIRECT_RX : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_ERROR : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_READY : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_RESET : gr55xx_hal_qspi.h
- HAL_RNG_STATE_BUSY : gr55xx_hal_rng.h
- HAL_RNG_STATE_ERROR : gr55xx_hal_rng.h
- HAL_RNG_STATE_READY : gr55xx_hal_rng.h
- HAL_RNG_STATE_RESET : gr55xx_hal_rng.h
- HAL_RNG_STATE_TIMEOUT : gr55xx_hal_rng.h
- HAL_SPI_STATE_ABORT : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_RX : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_TX : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_TX_RX : gr55xx_hal_spi.h
- HAL_SPI_STATE_ERROR : gr55xx_hal_spi.h
- HAL_SPI_STATE_READY : gr55xx_hal_spi.h
- HAL_SPI_STATE_RESET : gr55xx_hal_spi.h
- HAL_TIMEOUT : gr55xx_hal_def.h
- HAL_TIMER_STATE_BUSY : gr55xx_hal_tim.h
- HAL_TIMER_STATE_ERROR : gr55xx_hal_tim.h
- HAL_TIMER_STATE_READY : gr55xx_hal_tim.h
- HAL_TIMER_STATE_RESET : gr55xx_hal_tim.h
- HAL_UART_STATE_BUSY : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_RX : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_TX : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_TXRX : gr55xx_hal_uart.h
- HAL_UART_STATE_ERROR : gr55xx_hal_uart.h
- HAL_UART_STATE_READY : gr55xx_hal_uart.h
- HAL_UART_STATE_RESET : gr55xx_hal_uart.h
- HAL_UART_STATE_TIMEOUT : gr55xx_hal_uart.h
- HAL_UNLOCKED : gr55xx_hal_def.h
- HAL_XQSPI_STATE_ABORT : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY_INDIRECT_RX : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_ERROR : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_READY : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_RESET : gr55xx_hal_xqspi.h
- HIDS_EVT_BOOT_MODE_ENTERED : hids.h
- HIDS_EVT_HOST_EXIT_SUSP : hids.h
- HIDS_EVT_HOST_SUSP : hids.h
- HIDS_EVT_IN_REP_NOTIFY_DISABLED : hids.h
- HIDS_EVT_IN_REP_NOTIFY_ENABLED : hids.h
- HIDS_EVT_INVALID : hids.h
- HIDS_EVT_REP_CHAR_WRITE : hids.h
- HIDS_EVT_REPORT_MODE_ENTERED : hids.h
- HIDS_REPORT_TYPE_FEATURE : hids.h
- HIDS_REPORT_TYPE_IN1 : hids.h
- HIDS_REPORT_TYPE_IN2 : hids.h
- HIDS_REPORT_TYPE_IN3 : hids.h
- HIDS_REPORT_TYPE_KB_IN : hids.h
- HIDS_REPORT_TYPE_KB_OUT : hids.h
- HIDS_REPORT_TYPE_MOUSE_IN : hids.h
- HIDS_REPORT_TYPE_OUT : hids.h
- HIDS_REPORT_TYPE_RESERVED : hids.h
- HRRCPS_CTRL_PT_HRS_CONN_STA_REPORT : hrrcps.h
- HRRCPS_CTRL_PT_HRS_DISCONN : hrrcps.h
- HRRCPS_CTRL_PT_HRS_NTF_DISABLE : hrrcps.h
- HRRCPS_CTRL_PT_HRS_NTF_ENABLE : hrrcps.h
- HRRCPS_CTRL_PT_HRS_SEN_LOC_READ : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_CONN_STA_REPORT : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_DISCONN : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_NTF_DISABLE : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_NTF_ENABLE : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_SEN_LOC_READ : hrrcps.h
- HRRCPS_CTRL_PT_RSP_CODE : hrrcps.h
- HRRCPS_CTRL_PT_SCAN_HRS : hrrcps.h
- HRRCPS_CTRL_PT_SCAN_RSCS : hrrcps.h
- HRRCPS_EVT_CTRL_PT_IND_DISABLE : hrrcps.h
- HRRCPS_EVT_CTRL_PT_IND_ENABLE : hrrcps.h
- HRRCPS_EVT_DISABLE_HRS_NTF : hrrcps.h
- HRRCPS_EVT_DISABLE_RSCS_NTF : hrrcps.h
- HRRCPS_EVT_DISCONN_HRS_LINK : hrrcps.h
- HRRCPS_EVT_DISCONN_RSCS_LINK : hrrcps.h
- HRRCPS_EVT_ENABLE_HRS_NTF : hrrcps.h
- HRRCPS_EVT_ENABLE_RSCS_NTF : hrrcps.h
- HRRCPS_EVT_HRS_SENSOR_LOC_READ : hrrcps.h
- HRRCPS_EVT_INVALID : hrrcps.h
- HRRCPS_EVT_RSCS_SENSOR_LOC_READ : hrrcps.h
- HRRCPS_EVT_SCAN_HRS : hrrcps.h
- HRRCPS_EVT_SCAN_RSCS : hrrcps.h
- HRRCPS_RSP_ID_ERROR : hrrcps.h
- HRRCPS_RSP_ID_OK : hrrcps.h
- HRS_C_BIT_ENERGY_EXPENDED_STATUS : hrs_c.h
- HRS_C_BIT_INTERVAL : hrs_c.h
- HRS_C_BIT_RATE_FORMAT : hrs_c.h
- HRS_C_BIT_SENSOR_CONTACT_DETECTED : hrs_c.h
- HRS_C_BIT_SENSOR_CONTACT_SUPPORTED : hrs_c.h
- HRS_C_EVT_CTRL_POINT_SET : hrs_c.h
- HRS_C_EVT_DISCOVERY_COMPLETE : hrs_c.h
- HRS_C_EVT_DISCOVERY_FAIL : hrs_c.h
- HRS_C_EVT_HR_MEAS_NTF_SET_SUCCESS : hrs_c.h
- HRS_C_EVT_HR_MEAS_VAL_RECEIVE : hrs_c.h
- HRS_C_EVT_INVALID : hrs_c.h
- HRS_C_EVT_SENSOR_LOC_READ_RSP : hrs_c.h
- HRS_C_EVT_WRITE_OP_ERR : hrs_c.h
- HRS_C_SENS_LOC_CHEST : hrs_c.h
- HRS_C_SENS_LOC_EARLOBE : hrs_c.h
- HRS_C_SENS_LOC_FINGER : hrs_c.h
- HRS_C_SENS_LOC_FOOT : hrs_c.h
- HRS_C_SENS_LOC_HAND : hrs_c.h
- HRS_C_SENS_LOC_OTHER : hrs_c.h
- HRS_C_SENS_LOC_WRIST : hrs_c.h
- HRS_EVT_NOTIFICATION_DISABLED : hrs.h
- HRS_EVT_NOTIFICATION_ENABLED : hrs.h
- HRS_EVT_READ_BODY_SEN_LOCATION : hrs.h
- HRS_EVT_RESET_ENERGY_EXPENDED : hrs.h
- HRS_SENS_LOC_CHEST : hrs.h
- HRS_SENS_LOC_EARLOBE : hrs.h
- HRS_SENS_LOC_FINGER : hrs.h
- HRS_SENS_LOC_FOOT : hrs.h
- HRS_SENS_LOC_HAND : hrs.h
- HRS_SENS_LOC_OTHER : hrs.h
- HRS_SENS_LOC_WRIST : hrs.h
- HTS_EVT_INTM_TEM_NOTIFICATION_DISABLE : hts.h
- HTS_EVT_INTM_TEM_NOTIFICATION_ENABLE : hts.h
- HTS_EVT_INVALID : hts.h
- HTS_EVT_MEAS_INTERVAL_INDICATION_DISABLE : hts.h
- HTS_EVT_MEAS_INTERVAL_UPDATE : hts.h
- HTS_EVT_MEAS_INTREVAL_INDICATION_ENABLE : hts.h
- HTS_EVT_READ_CHARACTERISTIC : hts.h
- HTS_EVT_TEM_MEAS_INDICATION_DISABLE : hts.h
- HTS_EVT_TEM_MEAS_INDICATION_ENABLE : hts.h
- HTS_MEAS_FLAG_TEM_TYPE_BIT : hts.h
- HTS_MEAS_FLAG_TEM_UINTS_BIT : hts.h
- HTS_MEAS_FLAG_TIME_STAMP_BIT : hts.h
- HTS_READ_CHAR_MEAS_INTL : hts.h
- HTS_READ_CHAR_TEMP_TYPE : hts.h
- HTS_TEMP_TYPE_ARMPIT : hts.h
- HTS_TEMP_TYPE_BODY : hts.h
- HTS_TEMP_TYPE_EAR : hts.h
- HTS_TEMP_TYPE_EAR_DRUM : hts.h
- HTS_TEMP_TYPE_FINGER : hts.h
- HTS_TEMP_TYPE_GI_TRACT : hts.h
- HTS_TEMP_TYPE_MOUTH : hts.h
- HTS_TEMP_TYPE_RECTUM : hts.h
- HTS_TEMP_TYPE_TOE : hts.h
- HTS_TEMPERATURE_CELCIUS : hts.h
- HTS_TEMPERATURE_FAHRENHEIT : hts.h
- HTS_TEMPERATURE_INTERMEDIATE : hts.h
- HTS_TEMPERATURE_STABLE : hts.h