Macros
GPIO0_PIN8 MUX selection
Peripheral Driver » HAL Driver » GPIOEx » Defines » GPIOEx Exported Constants » GPIOEx Mux function selection

## Macros
#define | GPIO0_PIN8_MUX_XQSPIM_IO_0 GPIO_MUX_0
#define | GPIO0_PIN8_MUX_I2C1_SDA GPIO_MUX_1
#define | GPIO0_PIN8_MUX_QSPIM1_IO_0 GPIO_MUX_2
#define | GPIO0_PIN8_MUX_UART1_RX GPIO_MUX_3
#define | GPIO0_PIN8_MUX_PWM1_B GPIO_MUX_5

## Detailed Description

## Macro Definition Documentation

## ◆ GPIO0_PIN8_MUX_I2C1_SDA

#define GPIO0_PIN8_MUX_I2C1_SDA GPIO_MUX_1

GPIO0_PIN8 Mux Select I2C1_SDA

Definition at line 205 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN8_MUX_PWM1_B

#define GPIO0_PIN8_MUX_PWM1_B GPIO_MUX_5

GPIO0_PIN8 Mux Select PWM1_B

Definition at line 208 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN8_MUX_QSPIM1_IO_0

#define GPIO0_PIN8_MUX_QSPIM1_IO_0 GPIO_MUX_2

GPIO0_PIN8 Mux Select QSPIM1_IO_0

Definition at line 206 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN8_MUX_UART1_RX

#define GPIO0_PIN8_MUX_UART1_RX GPIO_MUX_3

GPIO0_PIN8 Mux Select UART1_RX

Definition at line 207 of file gr55xx_hal_gpio_ex.h.

## ◆ GPIO0_PIN8_MUX_XQSPIM_IO_0

#define GPIO0_PIN8_MUX_XQSPIM_IO_0 GPIO_MUX_0

GPIO0_PIN8 Mux Select XQSPIM_IO_0

Definition at line 204 of file gr55xx_hal_gpio_ex.h.