Macros
OTAS UUIDs
BLE Services » OTA Service Client (OTAS_C) » Defines

OTAS service and characteristcs UUID. More...

## Macros
#define | OTAS_SVC_UUID
#define | OTAS_TX_CHAR_UUID
#define | OTAS_RX_CHAR_UUID
#define | OTAS_CTRL_CHAR_UUID

## Detailed Description

OTAS service and characteristcs UUID.

## Macro Definition Documentation

## ◆ OTAS_CTRL_CHAR_UUID

#define OTAS_CTRL_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80, \
0x0A, 0x46, 0x44, 0xD3, 0x04, 0x04, 0xED, 0xA6}

UUID of OTA Control Characteristic.

Definition at line 82 of file otas_c.h.

## ◆ OTAS_RX_CHAR_UUID

#define OTAS_RX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80, \
0x0A, 0x46, 0x44, 0xD3, 0x03, 0x04, 0xED, 0xA6}

UUID of OTA RX Characteristic.

Definition at line 80 of file otas_c.h.

## ◆ OTAS_SVC_UUID

#define OTAS_SVC_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80, \
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x04, 0xED, 0xA6}

UUID of OTA Service.

Definition at line 76 of file otas_c.h.

## ◆ OTAS_TX_CHAR_UUID

#define OTAS_TX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80, \
0x0A, 0x46, 0x44, 0xD3, 0x02, 0x04, 0xED, 0xA6}

UUID of OTA TX Characteristic.

Definition at line 78 of file otas_c.h.