### - p -

- pass_alert_status_set() : pass.h
- pass_c_alert_status_notify_set() : pass_c.h
- pass_c_alert_status_read() : pass_c.h
- pass_c_ctrl_point_set() : pass_c.h
- pass_c_disc_srvc_start() : pass_c.h
- pass_c_ringer_set_notify_set() : pass_c.h
- pass_c_ringer_set_read() : pass_c.h
- pass_client_init() : pass_c.h
- pass_ringer_setting_get() : pass.h
- pass_ringer_setting_set() : pass.h
- pass_service_init() : pass.h
- pcs_service_init() : pcs.h
- pcs_setting_reply() : pcs.h
- pcs_tx_data_send() : pcs.h
- platform_clock_init() : platform_sdk.h
- platform_clock_init_rng() : platform_sdk.h
- platform_flash_enable_quad() : platform_sdk.h
- platform_flash_protection() : platform_sdk.h
- platform_init() : platform_sdk.h
- platform_init_pop() : platform_sdk.h
- platform_init_push() : platform_sdk.h
- platform_interrupt_protection_pop() : platform_sdk.h
- platform_interrupt_protection_push() : platform_sdk.h
- platform_rng2_calibration_get() : platform_sdk.h
- platform_rng2_calibration_is_busy() : platform_sdk.h
- platform_rng2_calibration_start() : platform_sdk.h
- platform_rng2_calibration_stop() : platform_sdk.h
- platform_sdk_init() : platform_sdk.h
- platform_set_rtc_crystal_delay() : platform_sdk.h
- pmu_calibration_handler() : platform_sdk.h
- prf_find_handle_by_idx() : ble_prf_utils.h
- prf_find_idx_by_handle() : ble_prf_utils.h
- prf_is_cccd_value_valid() : ble_prf_utils.h
- prf_is_indication_enabled() : ble_prf_utils.h
- prf_is_notification_enabled() : ble_prf_utils.h
- prf_pack_char_pres_fmt() : ble_prf_utils.h
- prf_pack_date_time() : ble_prf_utils.h
- prf_unpack_char_pres_fmt() : ble_prf_utils.h
- prf_unpack_date_time() : ble_prf_utils.h
- pwr_enter_sleep_check() : app_pwr_mgmt.h
- pwr_mgmt_baseband_state_get() : gr55xx_pwr.h
- pwr_mgmt_ble_wakeup() : gr55xx_pwr.h
- pwr_mgmt_check_ble_event() : gr55xx_pwr.h
- pwr_mgmt_check_ext_timer() : gr55xx_pwr.h
- pwr_mgmt_check_pend_irq() : gr55xx_pwr.h
- pwr_mgmt_dev_init() : gr55xx_pwr.h
- pwr_mgmt_dev_resume() : gr55xx_pwr.h
- pwr_mgmt_dev_suspend() : gr55xx_pwr.h
- pwr_mgmt_disable_nvic_irq() : gr55xx_pwr.h
- pwr_mgmt_enable_nvic_irq() : gr55xx_pwr.h
- pwr_mgmt_get_sleep_mode() : gr55xx_pwr.h
- pwr_mgmt_get_wakeup_flag() : gr55xx_pwr.h
- pwr_mgmt_init() : gr55xx_pwr.h
- pwr_mgmt_load_context() : gr55xx_pwr.h
- pwr_mgmt_mem_ctl_set() : gr55xx_pwr.h
- pwr_mgmt_mode_get() : gr55xx_pwr.h
- pwr_mgmt_mode_set() : gr55xx_pwr.h
- pwr_mgmt_notify_timer_event() : gr55xx_pwr.h
- pwr_mgmt_register_io_dump_func() : gr55xx_pwr.h
- pwr_mgmt_register_trace_func() : gr55xx_pwr.h
- pwr_mgmt_save_context() : gr55xx_pwr.h
- pwr_mgmt_schedule() : gr55xx_pwr.h
- pwr_mgmt_set_callback() : gr55xx_pwr.h
- pwr_mgmt_set_wakeup_flag() : gr55xx_pwr.h
- pwr_mgmt_shutdown() : gr55xx_pwr.h
- pwr_mgmt_ultra_sleep() : gr55xx_pwr.h
- pwr_mgmt_update_wkup_param() : gr55xx_pwr.h
- pwr_mgmt_wakeup_source_clear() : gr55xx_pwr.h
- pwr_mgmt_wakeup_source_setup() : gr55xx_pwr.h
- pwr_mgmt_warm_boot() : platform_sdk.h
- pwr_mgmt_wfe_sleep() : gr55xx_pwr.h
- pwr_register_sleep_cb() : app_pwr_mgmt.h
- pwr_unregister_sleep_cb() : app_pwr_mgmt.h
- pwr_wake_up_ind() : app_pwr_mgmt.h