Modules | Macros
MSIOEx Mux function selection
Peripheral Driver » HAL Driver » MSIOEx » Defines » MSIOEx Exported Constants

## Modules
| MSIO PIN common MUX selection(Available for all MSIO pins)
| MSIO_PIN0 MUX selection
| MSIO_PIN1 MUX selection
| MSIO_PIN2 MUX selection
| MSIO_PIN3 MUX selection
| MSIO_PIN4 MUX selection

## Macros
#define | IS_MSIO_MUX(__MUX__) (((__MUX__) <= MSIO_MUX_7))
| Check if MSIO mux mode is valid. More...

## Detailed Description

## Macro Definition Documentation

## ◆ IS_MSIO_MUX

#define IS_MSIO_MUX | ( |  | __MUX__ | ) | (((__MUX__) <= MSIO_MUX_7))

Check if MSIO mux mode is valid.

Parameters

  __MUX__ | MSIO mux mode.

Return values

  SET | (__ACTION__ is valid) or RESET (__ACTION__ is invalid)

Definition at line 154 of file gr55xx_hal_msio_ex.h.