Public Attributes | List of all members
_i2c_init Struct Reference
Peripheral Driver » HAL Driver » I2C » Structures » I2C Configuration

I2C Configuration Structure definition. More...

`#include <gr55xx_hal_i2c.h>`

## Public Attributes
uint32_t | speed
uint32_t | own_address
uint32_t | addressing_mode
uint32_t | general_call_mode

## Detailed Description

I2C Configuration Structure definition.

Definition at line 166 of file gr55xx_hal_i2c.h.

## Member Data Documentation

## ◆ addressing_mode

uint32_t _i2c_init::addressing_mode

Specifies if 7-bit or 10-bit addressing mode is selected. This parameter can be a value of I2C Addressing Mode

Definition at line 174 of file gr55xx_hal_i2c.h.

## ◆ general_call_mode

uint32_t _i2c_init::general_call_mode

Specifies if general call mode is selected. This parameter can be a value of I2C General Call Addressing Mode

Definition at line 177 of file gr55xx_hal_i2c.h.

## ◆ own_address

uint32_t _i2c_init::own_address

Specifies the device own address. This parameter can be a 7-bit or 10-bit address.

Definition at line 171 of file gr55xx_hal_i2c.h.

## ◆ speed

uint32_t _i2c_init::speed

Specifies the I2C transfer speed. This parameter can be a value of I2C Transfer Speed

Definition at line 168 of file gr55xx_hal_i2c.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_i2c.h