Classes | Macros | Typedefs | Enumerations | Functions
cts.h File Reference

Current Time Service API. More...

`#include "gr_includes.h"`
`#include "custom_config.h"`
`#include "ble_prf_utils.h"`
`#include <stdint.h>`
`#include <stdbool.h>`

Go to the source code of this file.

## Classes
struct | cts_exact_time_256_t
| CTS Exact Time 256. More...
struct | cts_cur_time_t
| CTS Current Time value. More...
struct | cts_loc_time_info_t
| CTS Local Time Information. More...
struct | cts_ref_time_info_t
| CTS Reference Time Information. More...
struct | cts_updata_ref_time_info_t
| CTS Reference Time Updata Information. More...
struct | cts_adj_info_t
| CTS Adjust information. More...
struct | cts_evt_t
| Current Time Service event. More...
struct | cts_init_t
| Current Time Service init structure. This contains all option and data needed for initialization of the service. More...

## Macros
#define | CTS_CONNECTION_MAX 10
#define | CTS_CUR_TIME_VAL_LEN 10
#define | TOTAL_CTS_CUR_TIME_VAL_LEN 27
#define | CTS_LOC_TIME_INFO_VAL_LEN 2
#define | TOTAL_CTS_LOC_TIME_INFO_VAL_LEN 6
#define | CTS_REF_TIME_INFO_VAL_LEN 4
#define | CTS_TIME_YEAR_VALID_VAL_MIN 1582
#define | CTS_TIME_YEAR_VALID_VAL_MAX 9999
#define | CTS_TIME_ZONE_OFFSET_MIN -48
#define | CTS_TIME_ZONE_OFFSET_MAX 56
#define | CTS_TIME_ACCURACY_OUT_RANGE 254
#define | CTS_TIME_ACCURACT_UNKNOWN 255
#define | CTS_ERROR_FIELDS_IGNORED 0x80
#define | CTS_CHAR_MANDATORY 0x0f
#define | CTS_CHAR_LOC_TIME_INFO_SUP 0x30
#define | CTS_CHAR_REF_TIME_INFO_SUP 0xc0
#define | CTS_CHAR_FULL 0xff
#define | CTS_AR_NO_CHANGE (0x00 << 0)
#define | CTS_AR_MAUAL_TIME_UPDATE (0x01 << 0)
#define | CTS_AR_EXT_REF_TIME_UPDATE (0x01 << 1)
#define | CTS_AR_TIME_ZONE_CHANGE (0x01 << 2)
#define | CTS_AR_DST_CHANGE (0x01 << 3)

## Typedefs
typedef void(* | cts_evt_handler_t) (cts_evt_t *p_evt)
| Current Time Service event handler type. More...

## Enumerations
enum | cts_week_day_t { CTS_WEEK_UNKNOWN_DAY, CTS_WEEK_MONDAY, CTS_WEEK_TUSEDAY, CTS_WEEK_WEDNESDAY, CTS_WEEK_THURSDAT, CTS_WEEK_FRIDAY, CTS_WEEK_SATURDAY, CTS_WEEK_SUNDAY }
| Current Time Day of week. More...
enum | cts_dst_offset_t { CTS_DST_OFFSET_STANDAR_TIME = 0x00, CTS_DST_OFFSET_HALF_HOUR = 0x02, CTS_DST_OFFSET_DAYLIGHT_TIME = 0x04, CTS_DST_OFFSET_DOUB_DAYLIGHT_TIME = 0x08, CTS_DST_OFFSET_DOUB_UNKNOWED_TIME = 0xff }
| Local time information:Daylight Saving Time Offset. More...
enum | cts_ref_time_source_t { CTS_REF_TIME_SRC_UNKNOWN, CTS_REF_TIME_SRC_NET_TIME_PROTOCOL, CTS_REF_TIME_SRC_GPS, CTS_REF_TIME_SRC_RADIO_TIME_SIGNAL, CTS_REF_TIME_SRC_MANUAL, CTS_REF_TIME_SRC_ATOMIC_CLOCK, CTS_REF_TIME_SRC_CELLUAR_NET }
| Reference time information:Time Source. More...
enum | cts_evt_type_t { CTS_EVT_INVALID = 0x00, CTS_EVT_CUR_TIME_NOTIFICATION_ENABLED, CTS_EVT_CUR_TIME_NOTIFICATION_DISABLED, CTS_EVT_CUR_TIME_SET_BY_PEER, CTS_EVT_LOC_TIME_INFO_SET_BY_PEER }
| Current Time Service event type. More...

## Functions
sdk_err_t | cts_service_init (cts_init_t *p_cts_init)
| Initialize a Current Time Service instance and add in the DB. More...
void | cts_exact_time_get (cts_init_t *p_exact_time)
| Get exact time for user. More...
void | cts_exact_time_update (cts_init_t *p_cts_exact_time)
| Update exact time. More...
void | cts_cur_time_adjust (cts_adj_info_t *p_adj_info)
| Adjust current time. More...
sdk_err_t | cts_cur_time_send (uint8_t conn_idx, cts_cur_time_t *p_cur_time)
| Send Current Time if its notification has been enabled. More...
void | cts_c_data_parse (uint8_t *p_data, uint16_t length)
| Data accepts data and processing functions. More...
void | reference_time_encode (uint8_t *p_data, uint16_t length)
| Serial port data is converted into reference time. More...
void | local_time_encode (uint8_t *p_data, uint8_t length)
| Serial port data is converted into local time. More...
void | current_time_encode (uint8_t *p_data, uint16_t length)
| Serial port data is converted into current time. More...
uint8_t | local_time_universal_decode (ble_gatts_write_cfm_t *p_cfm, cts_evt_t *p_evt)
| Handle Local Time Information conversion. More...
uint8_t | current_time_universal_decode (ble_gatts_write_cfm_t *p_cfm, cts_evt_t *p_evt)
| Decode for a Current Time. More...

## Detailed Description

Current Time Service API.

Attention
  #####Copyright (c) 2019 GOODIX All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file cts.h.