Enumerations
Enumerations
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control

## Enumerations
enum | ble_gap_get_conn_info_op_t { BLE_GAP_GET_CON_RSSI = 0, BLE_GAP_GET_CON_CHANNEL_MAP, BLE_GAP_GET_PHY, BLE_GAP_GET_CHAN_SEL_ALGO }
| The operation code used to get connection info. More...
enum | ble_gap_get_peer_info_op_t { BLE_GAP_GET_PEER_VERSION = 0, BLE_GAP_GET_PEER_FEATURES }
| The operation code used to get peer device info. More...
enum | ble_gap_ll_role_type_t { BLE_GAP_LL_ROLE_MASTER = 0, BLE_GAP_LL_ROLE_SLAVE = 1 }
| Device role of LL layer type. More...
enum | ble_gap_param_set_op_id_t { BLE_GAP_OPCODE_CHNL_MAP_SET, BLE_GAP_OPCODE_WHITELIST_SET, BLE_GAP_OPCODE_PER_ADV_LIST_SET, BLE_GAP_OPCODE_PRIVACY_MODE_SET }
| Operation code used to set param(s). More...
enum | ble_gap_psm_manager_op_id_t { BLE_GAP_OPCODE_LEPSM_REGISTER, BLE_GAP_OPCODE_LEPSM_UNREGISTER }
| Operation code used for LEPSM manager. More...
enum | ble_gap_disconn_reason_t { BLE_GAP_HCI_AUTHENTICATION_FAILURE = 0x05, BLE_GAP_HCI_REMOTE_USER_TERMINATED_CONNECTION = 0x13, BLE_GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_LOW_RESOURCES = 0x14, BLE_GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_POWER_OFF = 0x15, BLE_GAP_HCI_UNSUPPORTED_REMOTE_FEATURE = 0x1A, BLE_GAP_HCI_PAIRING_WITH_UNIT_KEY_UNSUPPORTED = 0X29, BLE_GAP_HCI_CONN_INTERVAL_UNACCEPTABLE = 0x3B }
| The specified reason for terminating a connection. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ ble_gap_disconn_reason_t

enum ble_gap_disconn_reason_t

The specified reason for terminating a connection.

Enumerator
BLE_GAP_HCI_AUTHENTICATION_FAILURE | Authentication Failure.
BLE_GAP_HCI_REMOTE_USER_TERMINATED_CONNECTION | Remote User Terminated Connection.
BLE_GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_LOW_RESOURCES | Remote Device Terminated Connection due to Low Resources .
BLE_GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_POWER_OFF | Remote Device Terminated Connection due to Power Off.
BLE_GAP_HCI_UNSUPPORTED_REMOTE_FEATURE | Unsupported Remote Feature.
BLE_GAP_HCI_PAIRING_WITH_UNIT_KEY_UNSUPPORTED | Pairing With Unit Key Not Supported.
BLE_GAP_HCI_CONN_INTERVAL_UNACCEPTABLE | Unacceptable Connection Parameters.

Definition at line 138 of file ble_gapc.h.

## ◆ ble_gap_get_conn_info_op_t

enum ble_gap_get_conn_info_op_t

The operation code used to get connection info.

Enumerator
BLE_GAP_GET_CON_RSSI | Get connection RSSI info.
BLE_GAP_GET_CON_CHANNEL_MAP | Get connection channel map.
BLE_GAP_GET_PHY | Get connection PHY.
BLE_GAP_GET_CHAN_SEL_ALGO | Get selection algorithm for connection channel.

Definition at line 93 of file ble_gapc.h.

## ◆ ble_gap_get_peer_info_op_t

enum ble_gap_get_peer_info_op_t

The operation code used to get peer device info.

Enumerator
BLE_GAP_GET_PEER_VERSION | Get peer device version info.
BLE_GAP_GET_PEER_FEATURES | Get peer device features info.

Definition at line 102 of file ble_gapc.h.

## ◆ ble_gap_ll_role_type_t

enum ble_gap_ll_role_type_t

Device role of LL layer type.

Enumerator
BLE_GAP_LL_ROLE_MASTER | Master role.
BLE_GAP_LL_ROLE_SLAVE | Slave role.

Definition at line 109 of file ble_gapc.h.

## ◆ ble_gap_param_set_op_id_t

enum ble_gap_param_set_op_id_t

Operation code used to set param(s).

Enumerator
BLE_GAP_OPCODE_CHNL_MAP_SET | Set Channel Map.
BLE_GAP_OPCODE_WHITELIST_SET | Set white list.
BLE_GAP_OPCODE_PER_ADV_LIST_SET | Set periodic advertising list.
BLE_GAP_OPCODE_PRIVACY_MODE_SET | Set privacy mode for peer device.

Definition at line 118 of file ble_gapc.h.

## ◆ ble_gap_psm_manager_op_id_t

enum ble_gap_psm_manager_op_id_t

Operation code used for LEPSM manager.

Enumerator
BLE_GAP_OPCODE_LEPSM_REGISTER | LEPSM register operation.
BLE_GAP_OPCODE_LEPSM_UNREGISTER | LEPSM unregister operation.

Definition at line 129 of file ble_gapc.h.