Macros
Parity Control
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants

## Macros
#define | LL_UART_PARITY_NONE UART_LCR_PARITY_NONE
#define | LL_UART_PARITY_ODD UART_LCR_PARITY_ODD
#define | LL_UART_PARITY_EVEN UART_LCR_PARITY_EVEN
#define | LL_UART_PARITY_SP0 UART_LCR_PARITY_SP0
#define | LL_UART_PARITY_SP1 UART_LCR_PARITY_SP1

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_PARITY_EVEN

#define LL_UART_PARITY_EVEN UART_LCR_PARITY_EVEN

Parity control enabled and Even Parity is selected

Definition at line 157 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_NONE

#define LL_UART_PARITY_NONE UART_LCR_PARITY_NONE

Parity control disabled

Definition at line 155 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_ODD

#define LL_UART_PARITY_ODD UART_LCR_PARITY_ODD

Parity control enabled and Odd Parity is selected

Definition at line 156 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_SP0

#define LL_UART_PARITY_SP0 UART_LCR_PARITY_SP0

Parity control enabled and Stick Parity 0 is selected

Definition at line 158 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_SP1

#define LL_UART_PARITY_SP1 UART_LCR_PARITY_SP1

Parity control enabled and Stick Parity 1 is selected

Definition at line 159 of file gr55xx_ll_uart.h.