Public Attributes | List of all members
gls_racp_filter_t Struct Reference
BLE Services » Glucose Service Record Access Control Point (GLS_RACP) » Structures

Glucose Recoerd Access Control Point filter value. More...

`#include <gls_racp.h>`

## Public Attributes
gls_racp_operator_t | racp_operator
gls_racp_filter_type_t | racp_filter_type
union {
struct {
uint16_t min
uint16_t max
} seq_num
struct {
prf_date_time_t min
prf_date_time_t max
} time
} | val

## Detailed Description

Glucose Recoerd Access Control Point filter value.

Definition at line 131 of file gls_racp.h.

## Member Data Documentation

## ◆ max [1/2]

uint16_t gls_racp_filter_t::max

Max sequence number.

Definition at line 140 of file gls_racp.h.

## ◆ max [2/2]

prf_date_time_t gls_racp_filter_t::max

Max base time.

Definition at line 145 of file gls_racp.h.

## ◆ min [1/2]

uint16_t gls_racp_filter_t::min

Min sequence number.

Definition at line 139 of file gls_racp.h.

## ◆ min [2/2]

prf_date_time_t gls_racp_filter_t::min

Min base time.

Definition at line 144 of file gls_racp.h.

## ◆ racp_filter_type

gls_racp_filter_type_t gls_racp_filter_t::racp_filter_type

Glucose Recoerd Access Control Point filter types.

Definition at line 134 of file gls_racp.h.

## ◆ racp_operator

gls_racp_operator_t gls_racp_filter_t::racp_operator

Glucose Recoerd Access Control Point Operator.

Definition at line 133 of file gls_racp.h.

## ◆ seq_num

struct { ... } gls_racp_filter_t::seq_num

Sequence number filtering (racp_filter_type = GLS_RACP_FILTER_SEQ_NUMBER).

## ◆ time

struct { ... } gls_racp_filter_t::time

User facing time filtering (filter_type = GLS_RACP_FILTER_USER_FACING_TIME).

## ◆ val

union { ... } gls_racp_filter_t::val

Filter union.

The documentation for this struct was generated from the following file:

- gls_racp.h