Public Attributes | List of all members
ags_ack_packet_t Struct Reference
BLE Services » Alexa Gadget Service (AGS) » Structures

Alexa Gadget Service ACK packet. More...

`#include <ags.h>`

## Public Attributes
ags_header_base_t | header_base
uint8_t | reserved_1
uint8_t | payload_length
uint8_t | reserved_2
uint8_t | result_code

## Detailed Description

Alexa Gadget Service ACK packet.

Definition at line 223 of file ags.h.

## Member Data Documentation

## ◆ header_base

ags_header_base_t ags_ack_packet_t::header_base

Header base.

Definition at line 225 of file ags.h.

## ◆ payload_length

uint8_t ags_ack_packet_t::payload_length

Length of the ACK packet.

Definition at line 227 of file ags.h.

## ◆ reserved_1

uint8_t ags_ack_packet_t::reserved_1

Reserved.

Definition at line 226 of file ags.h.

## ◆ reserved_2

uint8_t ags_ack_packet_t::reserved_2

Reserved.

Definition at line 228 of file ags.h.

## ◆ result_code

uint8_t ags_ack_packet_t::result_code

A result code, which depends on whether this is an ACK or a NACK. ags_header_ack_flag_t

Definition at line 229 of file ags.h.

The documentation for this struct was generated from the following file:

- ags.h